Quick Navigation
| Background
| System Summary
| Motherboard
| Processor
| BIOS
| PCI/AGP Devices
| Memory Modules
| Memory (SMBIOS)
| HDD
| ATAPI
| Storage (ASPI)
| Drives
| USB Devices
| Plug and Play
| Printers
| Slots (SMBIOS)
| Ports (SMBIOS)
| Monitor
| Video
Background
| Background
| Version | ASTRA v.5.41
| URL | www.sysinfolab.com
| Network Name | A2KKV_98
| Report Date | December 04, 2008
| Report Time | 13:24:02
| OS Version | MS Windows 98 SE (4.10.2222 A)
| Registered To | Sysinfo Lab
| License Type | Professional for 1 computer
System Summary
| Processor
| Processor | AMD Athlon 64 2800+
| CPU Clock | 2402.9 MHz (9.0 x 267.0 MHz)
| Level 1 Cache | 64+64 kB (data+instr.)
| Level 2 Cache | 512 kB
| Motherboard
| Motherboard Vendor | EPoX Computer Co., Ltd.
| BIOS Version | Phoenix - AwardBIOS v6.00PG
| Chipset Name | NVIDIA nForce3 250Gb
| Chipset Vendor | Nvidia Corp
| Chipset | nForce3 CPU to PCI Bridge
| Southbridge Vendor | Nvidia Corp
| Southbridge | nForce3 CPU to ISA Bridge
| PCI Bus Version | 2.10
| PnP BIOS Version | 1.0
| DMI/SMBIOS Version | 2.2
| Memory
| Base Memory | 640 kB (564 kB free)
| Extended Memory | 1045812 kB (1021.30 MB)
| System Memory | 1022 MB
| Memory Module | 512MB PC3200 DDR SDRAM (Samsung)
| Memory Module | 512MB PC3200 DDR SDRAM (Samsung)
| Storage
| Floppy Drive | A: 1.44 MB (3.5")
| HDD Model | Maxtor 7L300R0
| HDD Size | 286188 MB (279.48 GB)
| HDD Model | Kingston DataTraveler II+
| HDD Size | 491 MB (0.48 GB)
| CD/DVD Model | _NEC DVD_RW ND-3550A
| CD/DVD Speed | 48x (Write: 48x)
| CD/DVD Model | CD-W540E
| CD/DVD Speed | 48x (Write: 40x)
| Video
| Video Chip Vendor | Nvidia Corp
| Video Chip | GeForce 6800 [NV40.1]
| VESA OEM String | NVIDIA
| Video Memory Size | 128 MB
| Sound
| Sound Chip Vendor | Nvidia Corp
| Sound Chip | nForce3 AC'97 Audio Codec Interface
| AC'97/HDA Codec Name | Avance Logic ALC655
| Codec Enhancement | No 3D Stereo Enhancement
| Sound Chip Vendor | Creative Labs
| Sound Chip | EMU10K2 Audio Chipset (SB Audigy Series)
| Operating System
| DOS Version | Microsoft DOS 7.10 rev.0 in HMA
| Windows Version | MS Windows 98 SE (4.10.2222 A)
| Windows Folder | C:\WINDOWS
| Network
| Network Name | A2KKV_98
| Adapter Vendor | Nvidia Corp
| Adapter Name | Network Bus Enumerator
| MAC Address | 00-04-61-FF-FF-FE
| Ports
| Mouse Type | PS/2 (version 8.30)
| LPT Ports | LPT1(0378h)
| COM Ports | COM1(03F8h) COM2(02F8h)
| Joystick | Not Present
Motherboard
| System
| System Vendor |
| Product Name |
| Version |
| Serial Number |
| UUID | FFFFFFFFFFFFFFFFFFFFFFFFFFFFFFFF
| Wake-up Type | Power Switch
| Motherboard
| Motherboard Vendor | EPoX Computer Co., Ltd.
| Vendor URL | www.epox.com
| Board Model | nForce
| Version |
| Serial Number |
| BIOS Version | Phoenix - AwardBIOS v6.00PG
| BIOS Date | 05/02/06
| Chipset Name | NVIDIA nForce3 250Gb
| Chipset Vendor | Nvidia Corp
| Chipset | nForce3 CPU to PCI Bridge
| Southbridge Vendor | Nvidia Corp
| Southbridge | nForce3 CPU to ISA Bridge
| System Enclosure
| Manufacturer |
| Type | Desktop
| Version |
| Serial Number |
| Asset Tag |
| Boot-up State | Unknown
| Power Supply State | Unknown
| Thermal State | Unknown
| Security Status | Unknown
CPU
| CPU
| Processor | AMD Athlon 64 2800+
| Coprocessor | Internal
| CPU Clock | 2402.9 MHz
| Level 1 Cache | 64+64 kB (data+instr.)
| Level 2 Cache | 512 kB
| FSB Clock | 267.0 MHz
| Multiplier | 9.0
| Platform ID | Socket 754
| Vendor | AuthenticAMD
| Processor Name | AMD Athlon(tm) 64 Processor 2800+
| Processor Type | Original OEM Processor
| CPUID | Family: 15, Model: 12, Stepping: 0
| Ext. Family/Model | Family: 0, Model: 0
| CPU Signature | 00000FC0h
| Brand ID | Athlon 64 2800+ (0106h)
| Logical CPU Count | HTT Not Supported
| Max CPUID Level | 1
| Max ExtCPUID Level | 80000018h
| Code Name | Newcastle (0.13mk)
| Core Stepping | DH-CG
| MSR C0010015h | 00000000h:0A000000h
| MSR C0010042h | 00000202h:000A0A0Ah
| Instruction Set
| Floating-Point Unit On-Chip | Supported
| IA MMX Technology | Supported
| SSE Instruction Set | Supported
| SSE2 Instruction Set | Supported
| SSE3 Instruction Set | Not Supported
| Supplemental SSE3 Instruction Set | Not Supported
| SSE4.1 Instruction Set | Not Supported
| SSE4.2 Instruction Set | Not Supported
| Advanced Vector Extensions (AVX) | Not Supported
| FMA Instructions Set | Not Supported
| AES Instructions Set | Not Supported
| Intel Extended Memory 64 Tech. | Not Supported
| Intel Architecture - 64 (IA-64) | Not Supported
| AMD MMX Instruction Extensions | Supported
| AMD 3DNow! Instructions | Supported
| AMD 3DNow! Extensions | Supported
| AMD 3DNow! Prefetch | Not Supported
| AMD SSE4A Extensions | Not Supported
| AMD SSE5 Extensions | Not Supported
| AMD Misaligned SSE | Not Supported
| AMD64 Architecture | Supported
| Cyrix Extended MMX | Not Supported
| CMPXCHG8 Instruction Supported | Supported
| CMPXCHG16 Instruction Supported | Not Supported
| Fast System Call | Supported
| Conditional Move Instruction | Supported
| CLFLUSH Insruction Supported | Supported
| Fast Save and Restore | Supported
| Monitor/MWAIT Instructions | Not Supported
| SYSCALL/SYSRET Instructions | Supported
| LAHF/SAHF Instructions | Not Supported
| POPCNT Insruction Supported | Not Supported
| XSAVE Insructions Supported | Not Supported
| OS Supports XSAVE Instructions | Not Supported
| PCLMULQDQ Instruction Supported | Not Supported
| MOVBE Insruction Supported | Not Supported
| AMD RDTSCP Insruction Supported | Not Supported
| AMD Fast Save and Restore | Not Supported
| AMD SKINIT, STGI, DEV Supported | Not Supported
| Processor Features
| Virtual Mode Extension | Supported
| Debugging Extension | Supported
| Page Size Extension | Supported
| Time Stamp Counter | Supported
| Model Specific Registers | Supported
| Physical Address Extension | Supported
| Machine Check Exception | Supported
| On-chip APIC Hardware Supported | Supported
| Memory Type Range Registers | Supported
| Page Global Enable | Supported
| Machine Check Architecture | Supported
| Page Attribute Table | Supported
| 36-bit Page Size Extension | Supported
| Processor Serial Number | Not Supported
| Debug Store | Not Supported
| 64-bit Debug Store | Not Supported
| Self-Snoop | Not Supported
| Hyper-Threading Technology | Not Supported
| Pending Break Enable | Not Supported
| CPL-Qualified Debug Store | Not Supported
| L1 Context ID | Not Supported
| Send Task Priority Messages | Not Supported
| Direct Cache Access | Not Supported
| Performance Capabilities MSR | Not Supported
| x2APIC Architecture | Not Supported
| Advanced Bit Manipulation | Not Supported
| OS Visible Workaround | Not Supported
| Instruction Based Sampling | Not Supported
| Intel Virtualization Technology | Not Supported
| Intel Trusted Execution Technology | Not Supported
| Intel Turbo Boost Technology | Not Supported
| AMD No-execute Page Protection | Supported
| AMD Secure Virtual Machine | Not Supported
| AMD Model-Specific Registers | Supported
| AMD Multiprocessing Capable | Not Supported
| AMD CMP Legacy Mode | Not Supported
| AMD CR8 in Legacy Mode | Not Supported
| AMD Ext. APIC Register Space | Not Supported
| AMD Watchdog Timer | Not Supported
| AMD 1-GB Large Page | Not Supported
| Power Management
| ACPI Supported | Not Supported
| Thermal Monitor Supported | Not Supported
| Thermal Monitor 2 | Not Supported
| Enhanced SpeedStep Technology | Not Supported
| Digital Thermal Sensor | Not Supported
| Operating Point Protection | Not Supported
| AMD Temperature Sensor | Supported
| AMD Frequency ID Control | Supported
| AMD Voltage ID Control | Supported
| AMD Thermal Trip | Supported
| AMD Thermal Monitoring | Not Supported
| AMD Software Thermal Control | Not Supported
| AMD Invariant TSC | Not Supported
| AMD 100MHz Multiplier Steps | Not Supported
| AMD Hardware P-State Control | Not Supported
CPU Cache
| Level 1 Instruction Cache
| Size | 64 kB
| Associativity | 2-way
| Lines per Tag | 1
| Line Size | 64 byte
| TLB 4K Pages |
| Number of Entries | 32
| Associativity | full
| TLB 2/4M Pages |
| Number of Entries | 8
| Associativity | full
| Level 1 Data Cache
| Size | 64 kB
| Associativity | 2-way
| Lines per Tag | 1
| Line Size | 64 byte
| TLB 4K Pages |
| Number of Entries | 32
| Associativity | full
| TLB 2/4M Pages |
| Number of Entries | 8
| Associativity | full
| Level 2 Cache
| Size | 512 kB
| Associativity | 16-way
| Lines per Tag | 1
| Line Size | 64 byte
| Instr. TLB 4K Pages |
| Number of Entries | 512
| Associativity | 4-way
| Data TLB 4K Pages |
| Number of Entries | 512
| Associativity | 4-way
| Instr. TLB 2/4M Pages |
| Number of Entries | 0
| Associativity | off
| Data TLB 2/4M Pages |
| Number of Entries | 0
| Associativity | off
CPU (SMBIOS)
| Processor
| Processor Vendor | AMD
| Processor Version | AMD Athlon(tm) 64 Processor 2800+
| Current Speed | 2403 MHz
| External Clock | 267 MHz
| Voltage | 1.5 V
| Processor Upgrade | Socket 754
| Processor Status | CPU Enabled
| Socket Designation | Socket 754
| Processor Type | Central Processor
| Processor Family | AMD Opteron
| Processor ID1 | 00000FC0h
| Processor ID2 | 078BFBFFh
| Max Speed | 3000 MHz
| Socket Status | CPU Socket Populated
| Structure Length | 20h
CPU (SMBIOS) Cache
| Level 1 Cache
| Installed Size | 128 kB
| Operational Mode | Write Back
| Current SRAM Type | Synchronous
| Status | Enabled
| Socket Designation | Internal Cache
| Cache Socketed | Not Socketed
| Location | Internal
| Maximum Cache Size | 128 kB
| Supported SRAM Type | Synchronous
| Cache Speed | Unknown
| Error Correction | Unknown
| System Cache Type | Unknown
| Associativity | Unknown
| Structure Length | 13h
| Level 2 Cache
| Installed Size | 512 kB
| Operational Mode | Write Back
| Current SRAM Type | Synchronous
| Status | Enabled
| Socket Designation | External Cache
| Cache Socketed | Not Socketed
| Location | Internal
| Maximum Cache Size | 512 kB
| Supported SRAM Type | Synchronous
| Cache Speed | Unknown
| Error Correction | Unknown
| System Cache Type | Unknown
| Associativity | Unknown
| Structure Length | 13h
BIOS
| BIOS
| Motherboard Vendor | EPoX Computer Co., Ltd.
| Vendor URL | www.epox.com
| BIOS Version | Phoenix - AwardBIOS v6.00PG
| BIOS Model | Model: FCh SubModel: 01h Revision: 00h
| BIOS Date | 05/02/06
| BIOS Copyright | Phoenix Technologies, Ltd.- 04/23/90
| Motherboard ID | 05/02/2006 For nForce3 250 Chipset
| BIOS ID | 05/02/2006-nForce-6A61CPAFC-00
| BIOS Type | Medallion BIOS v6.00
| Bus Type | ISA/PCI
| Processor | 686
| Chipset | NVidia nForce3 150/250Gb
| Chipset ID | nForce
| BIOS Revision | 00
| MP Specification Ver. | 1.4
| MP Table Address | 000Fh:0C00h
| Number of CPU/Cores | 1
| DMI/SMBIOS Version | 2.2
| DMI/SMBIOS Structures | 34
| DMI/SMBIOS Address | 000Fh:0000h
| APM Version | Not Supported
| SMBIOS
| BIOS Vendor | Phoenix Technologies, LTD
| BIOS Version | 6.00 PG
| BIOS Date | 05/02/2006
| BIOS ROM Size | 512 kB
| Starting Segment | E000h
| Current Language | n|US|iso8859-1
| Number of Languages | 3
| Structure Length | 13h
| Bus Supported
| PCI is Supported | Supported
| AGP is Supported | Supported
| USB is Supported | Supported
| ISA is Supported | Supported
| VLBus is Supported | Not Supported
| MCA is Supported | Not Supported
| EISA is Supported | Not Supported
| PC Card is Supported | Not Supported
| Boot Options
| Selectable Boot | Supported
| Boot From CD | Supported
| ATAPI ZIP Drive Boot | Supported
| LS-120 Boot | Supported
| BIOS Boot Specification | Not Supported
| Boot From PC Card | Not Supported
| Network Service Boot Supported | Not Supported
| I2O Boot | Not Supported
| 1394 Boot | Not Supported
| BIOS Features
| BIOS Characteristics | Supported
| ACPI Supported | Supported
| PnP is Supported | Supported
| APM is Supported | Supported
| ESCD Support | Not Supported
| Enhanced Disk Drive (EDD) | Supported
| BIOS is Upgradeable (Flash) | Supported
| BIOS ROM is Socketed | Supported
| BIOS Shadowing is Allowed | Supported
| Smart Battery Supported | Not Supported
| Targeted Content Distribution | Not Supported
| Int 13h - 5.25"/360kB Floppy | Supported
| Int 13h - 5.25"/1.2MB Floppy | Supported
| Int 13h - 3.5"/720kB Floppy | Supported
| Int 13h - 3.5"/2.88MB Floppy | Supported
| Int 5h, Print Screen Service | Supported
| Int 9h, 8042 Keyboard Services | Supported
| Int 14h, Serial Services | Supported
| Int 17h, Printer Services | Supported
| Int 10h, CGA/Mono Video Services | Supported
| Int 13h - Floppy for NEC 9800 | Not Supported
| Int 13h - Floppy for Toshiba | Not Supported
| NEC PC-98 | Not Supported
| Other SMBIOS Structures
| Memory Array Mapped Address (19)
| Memory Device Mapped Address (20)
| Memory Device Mapped Address (20)
| System Boot Information (32)
PCI/AGP Devices
| PCI/AGP
| PCI Bus Version | 2.10
| Number of PCI Buses | 3
| Bus: 00h, Device: 00h, Function: 00h
| Vendor (10DEh) | Nvidia Corp
| Device (00E1h) | nForce3 CPU to PCI Bridge
| Subsys Vendor (1695h) | Epox Computer Co Ltd
| Subsystem ID (100Ch) | Unknown
| Class (06h) | Bridge
| SubClass (00h) | PCI/CPU
| Revision | A1h
| Interface | 00h
| Device Properties
| Device Timing | Fast
| Memory Access | Supported
| I/O Access | Not Supported
| Bus Master | Supported
| 66 MHz Speed Support | Supported
| Device Resources
| Memory Address | C0000000h - CFFFFFFFh
| AGP Capabilities
| AGP Version | 3.0
| AGP Speed Supported | 4x 8x (Selected: 8x)
| Fast Write | Supported, Enabled
| 4GB Addressing | Not Supported
| Side Band Addressing | Supported, Enabled
| Bus: 00h, Device: 01h, Function: 00h
| Vendor (10DEh) | Nvidia Corp
| Device (00E0h) | nForce3 CPU to ISA Bridge
| Subsys Vendor (1695h) | Epox Computer Co Ltd
| Subsystem ID (100Ch) | Unknown
| Class (06h) | Bridge
| SubClass (01h) | PCI/ISA
| Revision | A2h
| Interface | 00h
| Device Properties
| Device Timing | Fast
| Memory Access | Supported
| I/O Access | Supported
| Bus Master | Supported
| 66 MHz Speed Support | Supported
| Device Resources
| Bus: 00h, Device: 01h, Function: 01h
| Vendor (10DEh) | Nvidia Corp
| Device (00E4h) | nForce3 PCI SMB Controller
| Subsys Vendor (1695h) | Epox Computer Co Ltd
| Subsystem ID (100Ch) | Unknown
| Class (0Ch) | Serial
| SubClass (05h) | SMBus Controller
| Revision | A1h
| Interface | 00h
| Device Properties
| Device Timing | Fast
| Memory Access | Not Supported
| I/O Access | Supported
| Bus Master | Not Supported
| 66 MHz Speed Support | Supported
| Device Resources
| SMBus Port | 4C00h
| Base I/O Port | 0000E400h - 0000E41Fh
| Base I/O Port | 00004C00h - 00004C3Fh
| Base I/O Port | 00004C40h - 00004C7Fh
| System IRQ | 5
| Interrupt Pin | INTA#
| Bus: 00h, Device: 02h, Function: 00h
| Vendor (10DEh) | Nvidia Corp
| Device (00E7h) | nForce3 OHCI USB Controller
| Subsys Vendor (1695h) | Epox Computer Co Ltd
| Subsystem ID (100Ch) | Unknown
| Class (0Ch) | Serial
| SubClass (03h) | USB
| Revision | A1h
| Interface | 10h
| Device Properties
| Device Timing | Fast
| Memory Access | Supported
| I/O Access | Supported
| Bus Master | Supported
| 66 MHz Speed Support | Supported
| Device Resources
| Memory Address | DB004000h - DB004FFFh
| System IRQ | 5
| Interrupt Pin | INTA#
| Bus: 00h, Device: 02h, Function: 01h
| Vendor (10DEh) | Nvidia Corp
| Device (00E7h) | nForce3 OHCI USB Controller
| Subsys Vendor (1695h) | Epox Computer Co Ltd
| Subsystem ID (100Ch) | Unknown
| Class (0Ch) | Serial
| SubClass (03h) | USB
| Revision | A1h
| Interface | 10h
| Device Properties
| Device Timing | Fast
| Memory Access | Supported
| I/O Access | Supported
| Bus Master | Supported
| 66 MHz Speed Support | Supported
| Device Resources
| Memory Address | DB005000h - DB005FFFh
| System IRQ | 5
| Interrupt Pin | INTB#
| Bus: 00h, Device: 02h, Function: 02h
| Vendor (10DEh) | Nvidia Corp
| Device (00E8h) | nForce3 EHCI USB 2.0 Controller
| Subsys Vendor (1695h) | Epox Computer Co Ltd
| Subsystem ID (100Ch) | Unknown
| Class (0Ch) | Serial
| SubClass (03h) | USB
| Revision | A2h
| Interface | 20h
| Device Properties
| Device Timing | Fast
| Memory Access | Supported
| I/O Access | Not Supported
| Bus Master | Supported
| 66 MHz Speed Support | Supported
| Device Resources
| Memory Address | DB000000h - DB0000FFh
| System IRQ | 5
| Interrupt Pin | INTC#
| Bus: 00h, Device: 05h, Function: 00h
| Vendor (10DEh) | Nvidia Corp
| Device (00DFh) | Network Bus Enumerator
| Subsys Vendor (1695h) | Epox Computer Co Ltd
| Subsystem ID (100Ch) | Unknown
| Class (06h) | Bridge
| SubClass (80h) | PCI/Other
| Revision | A2h
| Interface | 00h
| Device Properties
| Device Timing | Fast
| Memory Access | Supported
| I/O Access | Supported
| Bus Master | Supported
| 66 MHz Speed Support | Supported
| Device Resources
| Memory Address | DB001000h - DB001FFFh
| Base I/O Port | 0000B800h - 0000B807h
| System IRQ | 5
| Interrupt Pin | INTA#
| Bus: 00h, Device: 06h, Function: 00h
| Vendor (10DEh) | Nvidia Corp
| Device (00EAh) | nForce3 AC'97 Audio Codec Interface
| Subsys Vendor (1695h) | Epox Computer Co Ltd
| Subsystem ID (100Dh) | Unknown
| Class (04h) | Multimedia
| SubClass (01h) | Audio
| Revision | A1h
| Interface | 00h
| Device Properties
| Device Timing | Fast
| Memory Access | Supported
| I/O Access | Supported
| Bus Master | Supported
| 66 MHz Speed Support | Supported
| Device Resources
| Base I/O Port | 0000BC00h - 0000BCFFh
| Base I/O Port | 0000C000h - 0000C07Fh
| Memory Address | DB002000h - DB002FFFh
| System IRQ | 11
| Interrupt Pin | INTA#
| AC'97/HDA Capabilities
| AC'97/HDA Codec Name | Avance Logic ALC655
| Codec Enhancement | No 3D Stereo Enhancement
| Bus: 00h, Device: 08h, Function: 00h
| Vendor (10DEh) | Nvidia Corp
| Device (00E5h) | nForce3 250 Parallel ATA Controller
| Subsys Vendor (1695h) | Epox Computer Co Ltd
| Subsystem ID (100Ch) | Unknown
| Class (01h) | Storage
| SubClass (01h) | IDE
| Revision | A2h
| Interface | 8Ah
| Device Properties
| Device Timing | Fast
| Memory Access | Not Supported
| I/O Access | Supported
| Bus Master | Supported
| 66 MHz Speed Support | Supported
| Device Resources
| Base I/O Port | 0000F000h - 0000F00Fh
| Bus: 00h, Device: 0Ah, Function: 00h
| Vendor (10DEh) | Nvidia Corp
| Device (00E3h) | nForce3 250 Serial ATA Controller
| Subsys Vendor (1695h) | Epox Computer Co Ltd
| Subsystem ID (100Ch) | Unknown
| Class (01h) | Storage
| SubClass (01h) | IDE
| Revision | A2h
| Interface | 85h
| Device Properties
| Device Timing | Fast
| Memory Access | Not Supported
| I/O Access | Supported
| Bus Master | Supported
| 66 MHz Speed Support | Supported
| Device Resources
| Base I/O Port | 000009F0h - 000009F7h
| Base I/O Port | 00000BF0h - 00000BF3h
| Base I/O Port | 00000970h - 00000977h
| Base I/O Port | 00000B70h - 00000B73h
| Base I/O Port | 0000DC00h - 0000DC0Fh
| Base I/O Port | 0000E000h - 0000E07Fh
| Bus: 00h, Device: 0Bh, Function: 00h
| Vendor (10DEh) | Nvidia Corp
| Device (00E2h) | nForce3 PCI to AGP Bridge
| Class (06h) | Bridge
| SubClass (04h) | PCI/PCI
| Revision | A2h
| Interface | 00h
| Device Properties
| Device Timing | Medium
| Memory Access | Supported
| I/O Access | Supported
| Bus Master | Supported
| 66 MHz Speed Support | Supported
| Device Resources
| Memory Address | D8000000h - DAFFFFFFh
| Memory Address | D0000000h - D7FFFFFFh
| Bus: 00h, Device: 0Eh, Function: 00h
| Vendor (10DEh) | Nvidia Corp
| Device (00EDh) | nForce3 PCI to PCI Bridge
| Class (06h) | Bridge
| SubClass (04h) | PCI/PCI
| Revision | A2h
| Interface | 00h
| Device Properties
| Device Timing | Fast
| Memory Access | Supported
| I/O Access | Supported
| Bus Master | Supported
| 66 MHz Speed Support | Supported
| Device Resources
| Base I/O Port | A000h - AFFFh
| Bus: 00h, Device: 18h, Function: 00h
| Vendor (1022h) | Advanced Micro Devices (AMD)
| Device (1100h) | Athlon64/Opteron/Sempron (K8 Family) HyperTransport Technology Configuration
| Class (06h) | Bridge
| SubClass (00h) | PCI/CPU
| Revision | 00h
| Interface | 00h
| Device Properties
| Device Timing | Fast
| Memory Access | Not Supported
| I/O Access | Not Supported
| Bus Master | Not Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Bus: 00h, Device: 18h, Function: 01h
| Vendor (1022h) | Advanced Micro Devices (AMD)
| Device (1101h) | Athlon64/Opteron/Sempron (K8 Family) Address Map
| Class (06h) | Bridge
| SubClass (00h) | PCI/CPU
| Revision | 00h
| Interface | 00h
| Device Properties
| Device Timing | Fast
| Memory Access | Not Supported
| I/O Access | Not Supported
| Bus Master | Not Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Bus: 00h, Device: 18h, Function: 02h
| Vendor (1022h) | Advanced Micro Devices (AMD)
| Device (1102h) | Athlon64/Opteron/Sempron (K8 Family) DRAM Controller
| Class (06h) | Bridge
| SubClass (00h) | PCI/CPU
| Revision | 00h
| Interface | 00h
| Device Properties
| Device Timing | Fast
| Memory Access | Not Supported
| I/O Access | Not Supported
| Bus Master | Not Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Bus: 00h, Device: 18h, Function: 03h
| Vendor (1022h) | Advanced Micro Devices (AMD)
| Device (1103h) | Athlon64/Opteron/Sempron (K8 Family) Miscellaneous Control
| Class (06h) | Bridge
| SubClass (00h) | PCI/CPU
| Revision | 00h
| Interface | 00h
| Device Properties
| Device Timing | Fast
| Memory Access | Not Supported
| I/O Access | Not Supported
| Bus Master | Not Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Bus: 01h, Device: 00h, Function: 00h
| Vendor (10DEh) | Nvidia Corp
| Device (0041h) | GeForce 6800 [NV40.1]
| Subsys Vendor (1043h) | ASUSTeK Computer Inc
| Subsystem ID (817Ch) | V9999 Ultra Deluxe
| Class (03h) | Display
| SubClass (00h) | VGA
| Revision | A1h
| Interface | 00h
| Device Properties
| Device Timing | Medium
| Memory Access | Supported
| I/O Access | Supported
| Bus Master | Supported
| 66 MHz Speed Support | Supported
| Device Resources
| Memory Address | D8000000h - D8FFFFFFh
| Memory Address | D0000000h - D7FFFFFFh
| Memory Address | D9000000h - D9FFFFFFh
| System IRQ | 11
| Interrupt Pin | INTA#
| AGP Capabilities
| AGP Version | 3.0
| AGP Speed Supported | 4x 8x (Selected: 8x)
| Fast Write | Supported, Enabled
| 4GB Addressing | Not Supported
| Side Band Addressing | Supported, Enabled
| Bus: 02h, Device: 0Bh, Function: 00h
| Vendor (1102h) | Creative Labs
| Device (0004h) | EMU10K2 Audio Chipset (SB Audigy Series)
| Subsys Vendor (1102h) | Creative Labs
| Subsystem ID (2005h) | Unknown
| Class (04h) | Multimedia
| SubClass (01h) | Audio
| Revision | 04h
| Interface | 00h
| Device Properties
| Device Timing | Medium
| Memory Access | Not Supported
| I/O Access | Supported
| Bus Master | Supported
| 66 MHz Speed Support | Not Supported
| Device Resources
| Base I/O Port | 0000A000h - 0000A03Fh
| System IRQ | 5
| Interrupt Pin | INTA#
Memory Modules
| Memory Slot 1
| Memory Type | 512MB PC3200 DDR SDRAM
| Manufacturer | Samsung
| Module Type | DIMM
| Number of Rows/Banks | 1 Rows, 4 Banks
| Module Attributes | Unbuffered
| Error Checking | None
| CAS# Latency | 3.0 (Cycle Time: 5.00ns/400MHz)
| CAS# Latency | 2.5 (Cycle Time: 6.00ns/333MHz)
| CS# Latency | 0
| WE# Latency | 1
| Refresh Rate | Reduced (0.5x) 7.8 us, Self Refresh
| Data Width | 64 bits
| SDRAM Width | x8
| Voltage Interface | SSTL 2.5 V
| SPD Revision | 1.0
| Part Number | M3 68L6523CUS-CCC
| Manufacture Date | May 2006 (0616h)
| Serial Number | F4253F48h
| Revision Code | 5343h
| EPP is Supported | Not Supported
| Memory Slot 2
| Memory Type | 512MB PC3200 DDR SDRAM
| Manufacturer | Samsung
| Module Type | DIMM
| Number of Rows/Banks | 1 Rows, 4 Banks
| Module Attributes | Unbuffered
| Error Checking | None
| CAS# Latency | 3.0 (Cycle Time: 5.00ns/400MHz)
| CAS# Latency | 2.5 (Cycle Time: 6.00ns/333MHz)
| CS# Latency | 0
| WE# Latency | 1
| Refresh Rate | Reduced (0.5x) 7.8 us, Self Refresh
| Data Width | 64 bits
| SDRAM Width | x8
| Voltage Interface | SSTL 2.5 V
| SPD Revision | 1.0
| Part Number | M3 68L6523DUS-CCC
| Manufacture Date | August 2006 (0622h)
| Serial Number | F42E570Eh
| Revision Code | 5344h
| EPP is Supported | Not Supported
Memory (SMBIOS)
| Physical Memory Array 1
| Maximum Capacity | 8192 MB
| Location | System Board or Motherboard
| Use | System Memory
| Memory Error Correct. | None
| Memory Devices | 2
| Structure Length | 0Fh
| Memory Device 1
| Size | 512 MB
| Form Factor | DIMM
| Memory Type | Unknown
| Device Locator | A0
| Bank Locator | Bank0/1
| Total Width | 64 bits
| Data Width | 64 bits
| Device Set | 00h
| Type Detail | None
| Structure Length | 15h
| Memory Device 2
| Size | 512 MB
| Form Factor | DIMM
| Memory Type | Unknown
| Device Locator | A1
| Bank Locator | Bank2/3
| Total Width | 64 bits
| Data Width | 64 bits
| Device Set | 00h
| Type Detail | None
| Structure Length | 15h
HDD
| Primary/Master HDD
| HDD Model | Maxtor 7L300R0
| HDD Size | 286188 MB (279.48 GB)
| Interface Type | Parallel ATA
| Geometry | Heads: 16, Sectors: 63, Tracks: 16383
| Compatibility | ATA/ATAPI-7 revision 30
| Serial Number | L61MYYGG
| Controller Revision | BAJ41G20
| HDD Marketing Size | 300090 MB (300.09 GB)
| Buffer Size | 16384.0 kB
| Buffer Type | Dual ported multi-sector buffer with a read caching
| HDD Temperature | 47 C (117 F)
| Reallocated Sectors | 0
| HDD Health Status | Good
| ECC bytes | 57
| Security Erase Time | None
| Enh. Security Erase | None
| Current APM Value | None
| Acoustic Management | FEh (C0h Recommended) - Enabled
| ATA Controller Vendor | Nvidia Corp
| ATA Controller Name | nForce3 250 Parallel ATA Controller
| Device Location | Primary/Master
| Transfer Modes
| PIO Mode Support | 4
| SW DMA Mode Support | Not Supported
| MW DMA Mode Support | 2, Active: None
| UDMA Mode Support | 6 (UltraDMA/133), Active: 6 (UltraDMA/133)
| Sectors per Interrupt | 16, Active: 16
| HDD Features
| SATA NCQ Command | Not Supported
| DMA Transfer | Supported
| LBA Supported | Supported
| Block Mode | Supported
| Double Word I/O | Not Supported
| Standard Standby Timer | Supported
| IORDY Supported | Supported
| IORDY may be Disabled | Supported
| S.M.A.R.T. | Supported, Enabled
| S.M.A.R.T. Self-test | Supported, Enabled
| S.M.A.R.T. Error Logging | Supported, Enabled
| Security Mode Feature Set | Supported, Disabled
| Removable Media | Not Supported
| Power Management | Supported, Enabled
| PACKET Command | Not Supported
| Write Cache | Supported, Enabled
| Look-ahead | Supported, Enabled
| Release Interrupt | Not Supported
| Service Interrupt | Not Supported
| Device Reset Command | Not Supported
| Host Protected Area | Supported, Enabled
| Write Verify Command | Supported, Enabled
| Write Buffer Command | Supported, Enabled
| Read Buffer Command | Supported, Enabled
| NOP Command | Supported, Enabled
| Identify Device DMA Command | Not Supported
| Download Microcode Command | Supported, Enabled
| Read/Write DMA Queued | Not Supported
| CFA Feature Set | Not Supported
| Advanced Power Management | Supported, Disabled
| Removable Media Status | Not Supported
| Power-up in Standby | Not Supported
| Set Features Req. to Spinup | Not Supported
| Set Max Security Extension | Supported, Disabled
| Automatic Acoustic Management | Supported, Enabled
| 48-bit Address | Supported, Enabled
| Device Configuration Overlay | Supported, Enabled
| Flush Cache Command | Supported, Enabled
| Flush Cache Ext Command | Supported, Enabled
| Media Serial Number | Not Supported
| Media Card Pass Through | Not Supported
| Streaming Feature Set | Supported, Disabled
| General Purpose Logging | Supported, Enabled
| Write DMA/Multiple FUA EXT | Supported, Enabled
| Write DMA Queued FUA EXT | Not Supported
| World Wide Name | Not Supported
| S.M.A.R.T.
| ID | Attribute Name | Threshold | Worst | Value | Raw Value
| 3 | Spin-up Time | 63 | 183 | 184 | 18579
| 4 | Start/Stop Count | 0 | 253 | 253 | 1665
| 5 | Reallocated Sectors Count | 63 | 253 | 253 | 0
| 6 | Read Channel Margin | 100 | 253 | 253 | 0
| 7 | Seek Error Rate | 0 | 252 | 253 | 0
| 8 | Seek Time Performance | 187 | 241 | 246 | 34507
| 9 | Power On Hours Count | 0 | 247 | 247 | 6750
| 10 | Spin-up Retry Count | 157 | 252 | 253 | 0
| 11 | Recalibration Retries | 223 | 252 | 253 | 0
| 12 | Drive Power Cycle Count | 0 | 249 | 249 | 1619
| 192 | Power-Off Retract Cycle | 0 | 253 | 253 | 0
| 193 | Load/Unload Cycle Count | 0 | 253 | 253 | 0
| 194 | Drive Temperature | 0 | 253 | 44 | 47
| 195 | Hardware ECC Recovered | 0 | 252 | 253 | 8381
| 196 | Reallocation Event Count | 0 | 253 | 253 | 0
| 197 | Current Pending Sectors | 0 | 253 | 253 | 0
| 198 | Uncorrectable Sectors | 0 | 253 | 253 | 0
| 199 | UltraDMA CRC Error Rate | 0 | 198 | 199 | 1
| 200 | Write Error Rate | 0 | 252 | 253 | 0
| 201 | Soft Read Error Rate | 0 | 252 | 253 | 0
| 202 | Data Address Mark Errors | 0 | 252 | 253 | 0
| 203 | Run Out Cancel | 180 | 252 | 253 | 0
| 204 | Soft ECC Correction | 0 | 252 | 253 | 0
| 205 | Thermal Asperity Rate | 0 | 252 | 253 | 0
| 207 | Spin High Current | 0 | 252 | 253 | 0
| 208 | Spin Buzz | 0 | 252 | 253 | 0
| 209 | Offline Seek Performance | 0 | 253 | 253 | 0
| 210 | Vibration During Write | 0 | 252 | 253 | 0
| 211 | Vibration During Read | 0 | 252 | 253 | 0
| 212 | Shock During Write | 0 | 252 | 253 | 0
ATAPI
| Secondary/Master ATAPI
| ATAPI Model | _NEC DVD_RW ND-3550A
| ATAPI Type | DVD+-RW DL/CD-RW
| Interface Type | Parallel ATA
| Physical Interface | ATAPI
| ATAPI Name | _NEC DVD_RW ND-3550A
| Vendor Specific | 05093000
| CD Read Speed | 48x (Current: 48x)
| CD Write Speed | 48x (Current: 48x)
| DVD Read Speed | Current: 6x
| DVD Write Speed | Current: 6x
| Buffer Size | 2048 kB
| Loading Mechanism | Tray Type
| Rotation Control | CLV
| Read Retry Count | 15
| Write Retry Count | 0
| Compatibility | Unknown
| Serial Number | 63E1J06S211
| Controller Revision | 1.05
| Command DRQ Type | Microprocessor DRQ
| Command Packet Size | 12 bytes
| ATA Controller Vendor | Nvidia Corp
| ATA Controller Name | nForce3 250 Parallel ATA Controller
| Device Location | Secondary/Master
| Transfer Modes
| PIO Mode Support | 4
| SW DMA Mode Support | Not Supported
| MW DMA Mode Support | 2, Active: None
| UDMA Mode Support | 2 (UltraDMA/33), Active: 2 (UltraDMA/33)
| Reading Features
| CD-R Disk Read | Supported
| CD-RW Disk Read | Supported
| DVD-ROM Disk Read | Supported
| DVD-RAM Disk Read | Not Supported
| DVD-R Disk Read | Supported
| DVD-R DL Disk Read | Supported
| DVD-RW Disk Read | Supported
| DVD-RW DL Disk Read | Not Supported
| DVD+R Disk Read | Supported
| DVD+R DL Disk Read | Supported
| DVD+RW Disk Read | Supported
| DVD+RW DL Disk Read | Not Supported
| BD-ROM Disk Read | Not Supported
| BD-R Disk Read | Not Supported
| BD-RE Disk Read | Not Supported
| HD DVD-ROM Disk Read | Not Supported
| HD DVD-RAM Disk Read | Not Supported
| HD DVD-R Disk Read | Not Supported
| HD DVD-R DL Disk Read | Not Supported
| HD DVD-RW Disk Read | Not Supported
| HD DVD-RW DL Disk Read | Not Supported
| Read Packet Using Method 2 | Supported
| Read Mode2 Form1 Sectors | Supported
| Read Mode2 Form2 Sectors | Supported
| Multisession Disk Read | Supported
| READ-CD Command on AudioCD | Supported
| Read Bar Code Capable | Not Supported
| Read Lead-in (CD-Text) | Supported
| Writing Features
| CD-R Disk Write | Supported
| CD-RW Disk Write | Supported
| DVD-RAM Disk Write | Not Supported
| DVD-R Disk Write | Supported
| DVD-R DL Disk Write | Supported
| DVD-RW Disk Write | Supported
| DVD+R Disk Write | Supported
| DVD+R DL Disk Write | Supported
| DVD+RW Disk Write | Supported
| DVD+RW DL Disk Write | Not Supported
| BD-R Disk Write | Not Supported
| BD-RE Disk Write | Not Supported
| HD DVD-R Disk Write | Not Supported
| HD DVD-R DL Disk Write | Not Supported
| HD DVD-RAM Disk Write | Not Supported
| HD DVD-RW Disk Write | Not Supported
| HD DVD-RW DL Disk Write | Not Supported
| Test Write Mode Support | Supported
| Buffer Underrun Protection | Supported
| Other Features
| Audio Play Support | Supported
| CD-DA Stream is Accurate | Supported
| Composite Audio/Video | Not Supported
| Digital Output on Port 1 | Not Supported
| Digital Output on Port 2 | Not Supported
| Support Subcode R-W | Supported
| Support Subcode R-W D&C | Not Supported
| C2 Pointers Supported | Supported
| ISRC Supported | Supported
| UPC Supported | Supported
| ATAPI Features
| DMA Transfer | Supported
| LBA Supported | Supported
| Block Mode | Not Supported
| IORDY Supported | Supported
| IORDY may be Disabled | Not Supported
| ATA Software Reset | Not Supported
| Overlap Operation | Not Supported
| Command Queuing | Not Supported
| Interleaving DMA | Not Supported
| Secondary/Slave ATAPI
| ATAPI Model | CD-W540E
| ATAPI Type | CD-RW
| Interface Type | Parallel ATA
| Physical Interface | ATAPI
| ATAPI Name | TEAC CD-W540E
| Vendor Specific | 09/30/02
| CD Read Speed | 48x (Current: 48x)
| CD Write Speed | 40x (Current: 40x)
| Buffer Size | 8192 kB
| Loading Mechanism | Tray Type
| Rotation Control | CLV
| Read Retry Count | 5
| Write Retry Count | 3
| Compatibility | ATA/ATAPI-5 revision 19
| Serial Number |
| Controller Revision | 1.0H
| Command DRQ Type | Accelerated DRQ
| Command Packet Size | 12 bytes
| ATA Controller Vendor | Nvidia Corp
| ATA Controller Name | nForce3 250 Parallel ATA Controller
| Device Location | Secondary/Slave
| Transfer Modes
| PIO Mode Support | 4
| SW DMA Mode Support | 2, Active: None
| MW DMA Mode Support | 2, Active: None
| UDMA Mode Support | 2 (UltraDMA/33), Active: 2 (UltraDMA/33)
| Reading Features
| CD-R Disk Read | Supported
| CD-RW Disk Read | Supported
| DVD-ROM Disk Read | Not Supported
| DVD-RAM Disk Read | Not Supported
| DVD-R Disk Read | Not Supported
| DVD-R DL Disk Read | Not Supported
| DVD-RW Disk Read | Not Supported
| DVD-RW DL Disk Read | Not Supported
| DVD+R Disk Read | Not Supported
| DVD+R DL Disk Read | Not Supported
| DVD+RW Disk Read | Not Supported
| DVD+RW DL Disk Read | Not Supported
| BD-ROM Disk Read | Not Supported
| BD-R Disk Read | Not Supported
| BD-RE Disk Read | Not Supported
| HD DVD-ROM Disk Read | Not Supported
| HD DVD-RAM Disk Read | Not Supported
| HD DVD-R Disk Read | Not Supported
| HD DVD-R DL Disk Read | Not Supported
| HD DVD-RW Disk Read | Not Supported
| HD DVD-RW DL Disk Read | Not Supported
| Read Packet Using Method 2 | Supported
| Read Mode2 Form1 Sectors | Supported
| Read Mode2 Form2 Sectors | Supported
| Multisession Disk Read | Supported
| READ-CD Command on AudioCD | Supported
| Read Bar Code Capable | Not Supported
| Read Lead-in (CD-Text) | Supported
| Writing Features
| CD-R Disk Write | Supported
| CD-RW Disk Write | Supported
| DVD-RAM Disk Write | Not Supported
| DVD-R Disk Write | Not Supported
| DVD-R DL Disk Write | Not Supported
| DVD-RW Disk Write | Not Supported
| DVD+R Disk Write | Not Supported
| DVD+R DL Disk Write | Not Supported
| DVD+RW Disk Write | Not Supported
| DVD+RW DL Disk Write | Not Supported
| BD-R Disk Write | Not Supported
| BD-RE Disk Write | Not Supported
| HD DVD-R Disk Write | Not Supported
| HD DVD-R DL Disk Write | Not Supported
| HD DVD-RAM Disk Write | Not Supported
| HD DVD-RW Disk Write | Not Supported
| HD DVD-RW DL Disk Write | Not Supported
| Test Write Mode Support | Supported
| Buffer Underrun Protection | Supported
| Other Features
| Audio Play Support | Supported
| CD-DA Stream is Accurate | Supported
| Composite Audio/Video | Not Supported
| Digital Output on Port 1 | Not Supported
| Digital Output on Port 2 | Not Supported
| Support Subcode R-W | Supported
| Support Subcode R-W D&C | Not Supported
| C2 Pointers Supported | Supported
| ISRC Supported | Supported
| UPC Supported | Supported
| ATAPI Features
| DMA Transfer | Supported
| LBA Supported | Supported
| Block Mode | Not Supported
| IORDY Supported | Supported
| IORDY may be Disabled | Supported
| ATA Software Reset | Not Supported
| Overlap Operation | Not Supported
| Command Queuing | Not Supported
| Interleaving DMA | Not Supported
| S.M.A.R.T. | Not Supported
| S.M.A.R.T. Self-test | Not Supported
| S.M.A.R.T. Error Logging | Not Supported
| Security Mode Feature Set | Not Supported
| Removable Media | Not Supported
| Power Management | Supported, Enabled
| PACKET Command | Supported, Enabled
| Write Cache | Not Supported
| Look-ahead | Not Supported
| Release Interrupt | Not Supported
| Service Interrupt | Not Supported
| Device Reset Command | Supported, Enabled
| Host Protected Area | Not Supported
| Write Verify Command | Not Supported
| Write Buffer Command | Not Supported
| Read Buffer Command | Not Supported
| NOP Command | Supported, Enabled
| Identify Device DMA Command | Not Supported
| Download Microcode Command | Not Supported
| Read/Write DMA Queued | Not Supported
| CFA Feature Set | Not Supported
| Advanced Power Management | Not Supported
| Removable Media Status | Not Supported
| Power-up in Standby | Not Supported
| Set Features Req. to Spinup | Not Supported
| Set Max Security Extension | Not Supported
| Automatic Acoustic Management | Not Supported
| 48-bit Address | Not Supported
| Device Configuration Overlay | Not Supported
| Flush Cache Command | Not Supported
| Flush Cache Ext Command | Not Supported
| Media Serial Number | Not Supported
| Media Card Pass Through | Not Supported
| Streaming Feature Set | Not Supported
| General Purpose Logging | Not Supported
| Write DMA/Multiple FUA EXT | Not Supported
| Write DMA Queued FUA EXT | Not Supported
| World Wide Name | Not Supported
Storage (ASPI)
| Host: 0, Target: 0, LUN: 0
| Device Name | Kingston DataTraveler II+
| Size | 491 MB (0.48 GB)
| Device Type | Disk Drive
| Compatibility | Not Standard
| Vendor Specific |
| Serial Number |
| Controller Revision | 1.13
| HDD Marketing Size | 515 MB (0.51 GB)
| Location | Host: 0, Target: 0, LUN: 0
| Manager ID | ASPI for Windows
| Adapter ID | PU20DISK
| Bus Width | 8-bit
| Address Width | 8-bit
| ASPI Device Features
| Removable Medium | Yes
| Read Cache | Not Supported
| Write Cache | Not Supported
| Read Reallocate | Not Supported
| Write Reallocate | Not Supported
| Terminate I/O Process | Not Supported
| Normal ACA | Not Supported
| Hierarchical Support | Not Supported
| Embedded Array Controller | Not Supported
| Protection Information | Not Supported
| Enclosure Services | Not Supported
| Multi-Ported Device | Not Supported
| Medium Changer | Not Supported
| Relative Addressing | Not Supported
| Synchronous Transfer | Not Supported
| Linked Commands | Not Supported
| Soft Reset | Not Supported
| Quick Arbitration | Not Supported
Drives
| BIOS Drives
| INT 13h Extensions | 1.x
| A:
| Drive Letter | A:
| Drive Size | 1.44 MB
| Drive Type | Floppy 1.44 MB (3.5")
| Cylinders | 80
| Heads | 2
| Sectors | 18
| C:
| Drive Letter | C:
| Drive Size | 286189 MB
| Drive Type | Fixed Disk
| Cylinders | 36483
| Heads | 255
| Sectors | 63
| D:
| Drive Letter | D:
| Drive Size | 490 MB
| Drive Type | Fixed Disk
| Cylinders | 490
| Heads | 64
| Sectors | 32
| H:
| Drive Letter | H:
| Drive Type | Optical Drive (MSCDEX Version: 2.95)
| I:
| Drive Letter | I:
| Drive Type | Optical Drive (MSCDEX Version: 2.95)
| Local Drives
| A:
| Drive Letter | A:
| Drive Type | Floppy 1.44 MB (3.5")
| C:[SYSTEM]
| Drive Letter | C:
| Drive Type | Fixed Disk
| Volume Label | SYSTEM
| File System | FAT16
| Volume Serial Number | 2255-1BEA
| Total Size | 2047.0 MB
| Free Space | 704.0 kB (0.0%)
| D:[UTILITIES]
| Drive Letter | D:
| Drive Type | Fixed Disk
| Volume Label | UTILITIES
| File System | FAT16
| Volume Serial Number | 2E4A-1BEB
| Total Size | 2047.0 MB
| Free Space | 7.5 MB (0.4%)
| E:[GAMES]
| Drive Letter | E:
| Drive Type | Fixed Disk
| Volume Label | GAMES
| File System | FAT16
| Volume Serial Number | 2D54-1BEC
| Total Size | 2047.0 MB
| Free Space | 21.2 MB (1.0%)
| F:[INSTALL]
| Drive Letter | F:
| Drive Type | Fixed Disk
| Volume Label | INSTALL
| File System | FAT16
| Volume Serial Number | 313D-1BED
| Total Size | 1890.2 MB
| Free Space | 436.6 MB (23.1%)
| G:[MUSIC]
| Drive Letter | G:
| Drive Type | Fixed Disk
| Volume Label | MUSIC
| File System | FAT32
| Volume Serial Number | B9FE-C68F
| Total Size | 115.0 GB
| Free Space | 143.3 MB (0.1%)
| H:
| Drive Letter | H:
| Drive Type | Optical Drive
| I:
| Drive Letter | I:
| Drive Type | Optical Drive
| K:[KINGSTON]
| Drive Letter | K:
| Drive Type | Removable Disk
| Volume Label | KINGSTON
| File System | FAT16
| Volume Serial Number | 94C6-CB33
| Total Size | 491.2 MB
| Free Space | 228.1 MB (46.4%)
USB Devices
| USB Device 1
| Vendor (0951h) | Kingston Technology
| Device (1601h) | DataTraveler II Plus
| Manufacturer | Kingston
| Product | DataTraveler II+
| Serial Number | 5B571621109C
| Device Version | 1.00
| Class (00h) | Unknown
| SubClass (00h) | Unknown
| Protocol (00h) | Unknown
| Configuration |
| USB Version | 2.00
| Speed | 480 Mb/s
| Transfer Type | Bulk
| Data Packet Size | 64 bytes
| Max Power | 200 mA
| Interface 1
| Class (08h) | Mass Storage
| SubClass (06h) | SCSI
| Protocol (50h) | Bulk (Zip)
| Interface |
Plug and Play
| Plug and Play
| PnP Version | 1.0
| Number of PnP Devices | 17
| Device Number 1
| PnP Device Name | AT Interrupt Controller
| PnP Device ID | PNP0000
| Base Type (08h) | System Peripheral
| SubType (00h) | Interrupt controller
| Node Size | 37 byte
| Device Resources
| I/O Port | 0020h-0021h
| I/O Port | 00A0h-00A1h
| System IRQ | 2 - High True Edge
| Device Number 2
| PnP Device Name | AT DMA Controller
| PnP Device ID | PNP0200
| Base Type (08h) | System Peripheral
| SubType (01h) | DMA controller
| Node Size | 69 byte
| Device Resources
| I/O Port | 0000h-000Fh
| I/O Port | 0081h-0083h
| I/O Port | 0087h-0087h
| I/O Port | 0089h-008Bh
| I/O Port | 008Fh-0091h
| I/O Port | 00C0h-00DFh
| DMA Channel | 4 - Type 8237 (8-bit)
| Device Number 3
| PnP Device Name | AT Timer
| PnP Device ID | PNP0100
| Base Type (08h) | System Peripheral
| SubType (02h) | System timer
| Node Size | 29 byte
| Device Resources
| I/O Port | 0040h-0043h
| System IRQ | 0 - High True Edge
| Device Number 4
| PnP Device Name | AT Real-Time Clock
| PnP Device ID | PNP0B00
| Base Type (08h) | System Peripheral
| SubType (03h) | Real Time Clock
| Node Size | 29 byte
| Device Resources
| I/O Port | 0070h-0071h
| System IRQ | 8 - High True Edge
| Device Number 5
| PnP Device Name | IBM Enhanced keyboard controller (101/2-key)
| PnP Device ID | PNP0303
| Base Type (09h) | Input Device
| SubType (00h) | Keyboard Controller
| Node Size | 37 byte
| Device Resources
| I/O Port | 0060h-0060h
| I/O Port | 0064h-0064h
| System IRQ | 1 - High True Edge
| Device Number 6
| PnP Device Name | AT standard speaker sound
| PnP Device ID | PNP0800
| Base Type (08h) | System Peripheral
| SubType (80h) | Other System device
| Node Size | 26 byte
| Device Resources
| I/O Port | 0061h-0061h
| Device Number 7
| PnP Device Name | Math Coprocessor
| PnP Device ID | PNP0C04
| Base Type (0Bh) | CPU Type
| SubType (01h) | 486 CPU
| Node Size | 29 byte
| Device Resources
| I/O Port | 00F0h-00FFh
| System IRQ | 13 - High True Edge
| Device Number 8
| PnP Device Name | System Board
| PnP Device ID | PNP0C01
| Base Type (05h) | Memory
| SubType (00h) | RAM Memory
| Node Size | 90 byte
| Device Resources
| Memory Address | 00000000h-FFFFFFFFh RAM 8-bit Cacheble
| Memory Address | FFFE0000h-FFFDFFFFh ROM 8/16-bit Cacheble
| Memory Address | FEC00000h-FEBFFFFFh ROM 8/16-bit Cacheble
| Memory Address | FEE00000h-FEDFFFFFh ROM 8/16-bit Cacheble
| Memory Address | FEFFFC00h-FEFFFFFFh ROM 8/16-bit Cacheble
| Memory Address | 00100000h-000FFFFFh RAM 8-bit Cacheble
| Device Number 9
| PnP Device Name | Motherboard registers
| PnP Device ID | PNP0C02
| Base Type (08h) | System Peripheral
| SubType (80h) | Other System device
| Node Size | 66 byte
| Device Resources
| Memory Address | 000F0000h-000F3FFFh ROM 8/16-bit Cacheble Shadow
| Memory Address | 000F4000h-000F7FFFh ROM 8/16-bit Cacheble Shadow
| Memory Address | 000F8000h-000FFFFFh ROM 8/16-bit Cacheble Shadow
| Memory Address | 000D5800h-000D7FFFh ROM 8/16-bit Cacheble Shadow
| Device Number 10
| PnP Device Name | PCI Bus
| PnP Device ID | PNP0A03
| Base Type (06h) | Bridge Controller
| SubType (04h) | PCI Bridge
| Node Size | 42 byte
| Device Resources
| I/O Port | 0294h-0297h
| I/O Port | 04D0h-04D1h
| I/O Port | 0CF8h-0CFFh
| Device Number 11
| PnP Device Name | PS/2 Port for PS/2-style Mice
| PnP Device ID | PNP0F13
| Base Type (09h) | Input Device
| SubType (02h) | Mouse Controller
| Node Size | 26 byte
| Device Resources
| System IRQ | 12 - High True Edge
| Device Number 12
| PnP Device Name | 16550A-compatible COM port
| PnP Device ID | PNP0501
| Base Type (07h) | Communications
| SubType (00h) | RS-232 Serial port
| Node Size | 69 byte
| Device Resources
| I/O Port | 03F8h-03FFh
| System IRQ | 4 - High True Edge
| Device Number 13
| PnP Device Name | PC standard floppy disk controller
| PnP Device ID | PNP0700
| Base Type (01h) | Mass Storage
| SubType (02h) | Floppy Controller
| Node Size | 64 byte
| Device Resources
| I/O Port | 03F0h-03F5h
| I/O Port | 03F7h-03F7h
| System IRQ | 6 - High True Edge
| DMA Channel | 2 - Type 8237 (8-bit)
| Device Number 14
| PnP Device Name | Standard LPT printer port
| PnP Device ID | PNP0400
| Base Type (07h) | Communications
| SubType (01h) | AT Parallel port
| Node Size | 92 byte
| Device Resources
| I/O Port | 0378h-037Fh
| I/O Port | 0778h-077Bh
| System IRQ | 7 - High True Edge
| Device Number 15
| PnP Device Name | 16550A-compatible COM port
| PnP Device ID | PNP0501
| Base Type (07h) | Communications
| SubType (00h) | RS-232 Serial port
| Node Size | 69 byte
| Device Resources
| I/O Port | 0000h-FFFFh
| Device Number 16
| PnP Device Name | MPU401 compatible
| PnP Device ID | PNPB006
| Base Type (04h) | Multimedia
| SubType (01h) | Audio controller
| Node Size | 60 byte
| Device Resources
| I/O Port | 0330h-0331h
| System IRQ | 10 - High True Edge
| Device Number 17
| PnP Device Name | Joystick/Game port
| PnP Device ID | PNPB02F
| Base Type (04h) | Multimedia
| SubType (01h) | Audio controller
| Node Size | 69 byte
| Device Resources
| I/O Port | 0201h-0207h
| I/O Port | 0200h-0200h
Physical Printers
| LPT/PnP or USB printer not found
Slots (SMBIOS)
| Slot PCI
| Slot Type | PCI
| Current Usage | Available
| Data Bus Width | 32 bit
| Slot Designation | PCI0
| Slot Length | Long Length
| Slot ID | 1
| Slot PCI
| Slot Type | PCI
| Current Usage | Available
| Data Bus Width | 32 bit
| Slot Designation | PCI1
| Slot Length | Long Length
| Slot ID | 2
| Slot PCI
| Slot Type | PCI
| Current Usage | Available
| Data Bus Width | 32 bit
| Slot Designation | PCI2
| Slot Length | Long Length
| Slot ID | 3
| Slot PCI
| Slot Type | PCI
| Current Usage | Available
| Data Bus Width | 32 bit
| Slot Designation | PCI3
| Slot Length | Long Length
| Slot ID | 4
| Slot PCI
| Slot Type | PCI
| Current Usage | Available
| Data Bus Width | 32 bit
| Slot Designation | PCI4
| Slot Length | Long Length
| Slot ID | 5
| Slot AGP
| Slot Type | AGP
| Current Usage | In Use
| Data Bus Width | 32 bit
| Slot Designation | AGP
| Slot Length | Long Length
| Slot ID | 88
Ports (SMBIOS)
| Port 1 Other
| Int. Connector Type | On Board IDE
| Ext. Connector Type | None
| Port Type | Other
| Int. Designator | PRIMARY IDE
| Ext. Designator |
| Port 2 Other
| Int. Connector Type | On Board IDE
| Ext. Connector Type | None
| Port Type | Other
| Int. Designator | SECONDARY IDE
| Ext. Designator |
| Port 3 8251 FIFO Compatible
| Int. Connector Type | On Board Floppy
| Ext. Connector Type | None
| Port Type | 8251 FIFO Compatible
| Int. Designator | FDD
| Ext. Designator |
| Port 4 Serial Port 16450 Compatible
| Int. Connector Type | 9 Pin Dual Inline (pin 10 cut)
| Ext. Connector Type | DB-9 pin male
| Port Type | Serial Port 16450 Compatible
| Int. Designator | COM1
| Ext. Designator |
| Port 5 Serial Port 16450 Compatible
| Int. Connector Type | 9 Pin Dual Inline (pin 10 cut)
| Ext. Connector Type | DB-9 pin male
| Port Type | Serial Port 16450 Compatible
| Int. Designator | COM2
| Ext. Designator |
| Port 6 Parallel Port ECP/EPP
| Int. Connector Type | DB-25 pin female
| Ext. Connector Type | DB-25 pin female
| Port Type | Parallel Port ECP/EPP
| Int. Designator | LPT1
| Ext. Designator |
| Port 7 Keyboard Port
| Int. Connector Type | PS/2
| Ext. Connector Type | PS/2
| Port Type | Keyboard Port
| Int. Designator | Keyboard
| Ext. Designator |
| Port 8 Mouse Port
| Int. Connector Type | PS/2
| Ext. Connector Type | PS/2
| Port Type | Mouse Port
| Int. Designator | PS/2 Mouse
| Ext. Designator |
| Port 9 USB
| Int. Connector Type | None
| Ext. Connector Type | Other
| Port Type | USB
| Int. Designator |
| Ext. Designator | USB0
Monitor
| PnP monitor not found
Video
| Video
| Video Chip Vendor | Nvidia Corp
| Video Chip | GeForce 6800 [NV40.1]
| Subsystem Vendor | ASUSTeK Computer Inc
| Subsystem ID | V9999 Ultra Deluxe
| Video Memory Size | 128 MB
| Bus Type | AGP
| VESA OEM String | NVIDIA
| VESA Version | 3.0
| Vendor Name | NVIDIA Corporation
| Product Name | nv40 Board - p212-0 Chip Rev
| OEM Software Version | 5.64
| VESA Power Management
| VESA PM Version | 1.0
| Standby | Supported
| Suspend | Supported
| Off | Supported
| Reduced On | Not Supported
| AGP Capabilities
| AGP Version | 3.0
| AGP Speed Supported | 4x 8x (Selected: 8x)
| Fast Write | Supported, Enabled
| 4GB Addressing | Not Supported
| Side Band Addressing | Supported, Enabled
| VESA Modes
| Number | Mode | Resolution | Colors | bpp | Features
| 100h | Graph | 640x400 | 256 | 8 | Bank + LFB
| 101h | Graph | 640x480 | 256 | 8 | Bank + LFB
| 102h | Graph | 800x600 | 16 | 4 | Bank
| 103h | Graph | 800x600 | 256 | 8 | Bank + LFB
| 104h | Graph | 1024x768 | 16 | 4 | Bank
| 105h | Graph | 1024x768 | 256 | 8 | Bank + LFB
| 10Eh | Graph | 320x200 | 64k | 16 | Bank + LFB
| 10Fh | Graph | 320x200 | 16M | 32 | Bank + LFB
| 111h | Graph | 640x480 | 64k | 16 | Bank + LFB
| 112h | Graph | 640x480 | 16M | 32 | Bank + LFB
| 114h | Graph | 800x600 | 64k | 16 | Bank + LFB
| 115h | Graph | 800x600 | 16M | 32 | Bank + LFB
| 117h | Graph | 1024x768 | 64k | 16 | Bank + LFB
| 118h | Graph | 1024x768 | 16M | 32 | Bank + LFB
| 130h | Graph | 320x200 | 256 | 8 | Bank + LFB
| 131h | Graph | 320x400 | 256 | 8 | Bank + LFB
| 132h | Graph | 320x400 | 64k | 16 | Bank + LFB
| 133h | Graph | 320x400 | 16M | 32 | Bank + LFB
| 134h | Graph | 320x240 | 256 | 8 | Bank + LFB
| 135h | Graph | 320x240 | 64k | 16 | Bank + LFB
| 136h | Graph | 320x240 | 16M | 32 | Bank + LFB
| 13Dh | Graph | 640x400 | 64k | 16 | Bank + LFB
| 13Eh | Graph | 640x400 | 16M | 32 | Bank + LFB