  +------------------------------------------------------------------------+
  |    This report is created by ASTRA v.5.41     Dec-04-2008 13:24:02     |
  +------------------------------------------------------------------------+
                               A2KKV_98

     Registered To:            Sysinfo Lab
     License Type:             Professional for 1 computer

                  +-----------------------------------------+
                  |              System Summary             |
                  +-----------------------------------------+
  Processor
     Processor:                AMD Athlon 64 2800+
     CPU Clock:                2402.9 MHz (9.0 x 267.0 MHz)
     Level 1 Cache:            64+64 kB (data+instr.)
     Level 2 Cache:            512 kB
  Motherboard
     Motherboard Vendor:       EPoX Computer Co., Ltd.
     BIOS Version:             Phoenix - AwardBIOS v6.00PG
     Chipset Name:             NVIDIA nForce3 250Gb
     Chipset Vendor:           Nvidia Corp
     Chipset:                  nForce3 CPU to PCI Bridge
     Southbridge Vendor:       Nvidia Corp
     Southbridge:              nForce3 CPU to ISA Bridge
     PCI Bus Version:          2.10
     PnP BIOS Version:         1.0
     DMI/SMBIOS Version:       2.2
  Memory
     Base Memory:              640 kB (564 kB free)
     Extended Memory:          1045812 kB (1021.30 MB)
     System Memory:            1022 MB
     Memory Module:            512MB PC3200 DDR SDRAM (Samsung)
     Memory Module:            512MB PC3200 DDR SDRAM (Samsung)
  Storage
     Floppy Drive:             A: 1.44 MB (3.5")
     HDD Model:                Maxtor 7L300R0
     HDD Size:                 286188 MB (279.48 GB)
     HDD Model:                Kingston DataTraveler II+
     HDD Size:                 491 MB (0.48 GB)
     CD/DVD Model:             _NEC DVD_RW ND-3550A
     CD/DVD Speed:             48x (Write: 48x)
     CD/DVD Model:             CD-W540E
     CD/DVD Speed:             48x (Write: 40x)
  Video
     Video Chip Vendor:        Nvidia Corp
     Video Chip:               GeForce 6800 [NV40.1]
     VESA OEM String:          NVIDIA
     Video Memory Size:        128 MB
  Sound
     Sound Chip Vendor:        Nvidia Corp
     Sound Chip:               nForce3 AC'97 Audio Codec Interface
     AC'97/HDA Codec Name:     Avance Logic ALC655
     Codec Enhancement:        No 3D Stereo Enhancement
     Sound Chip Vendor:        Creative Labs
     Sound Chip:               EMU10K2 Audio Chipset (SB Audigy Series)
  Operating System
     DOS Version:              Microsoft DOS 7.10 rev.0 in HMA
     Windows Version:          MS Windows 98 SE (4.10.2222 A)
     Windows Folder:           C:\WINDOWS
  Network
     Network Name:             A2KKV_98
     Adapter Vendor:           Nvidia Corp
     Adapter Name:             Network Bus Enumerator
     MAC Address:              00-04-61-FF-FF-FE
  Ports
     Mouse Type:               PS/2 (version 8.30)
     LPT Ports:                LPT1(0378h)
     COM Ports:                COM1(03F8h) COM2(02F8h)
     Joystick:                 Not Present

                  +-----------------------------------------+
                  |               Motherboard               |
                  +-----------------------------------------+
  System
     System Vendor:
     Product Name:
     Version:
     Serial Number:
     UUID:                     FFFFFFFFFFFFFFFFFFFFFFFFFFFFFFFF
     Wake-up Type:             Power Switch
  Motherboard
     Motherboard Vendor:       EPoX Computer Co., Ltd.
     Vendor URL:               www.epox.com
     Board Model:              nForce
     Version:
     Serial Number:
     BIOS Version:             Phoenix - AwardBIOS v6.00PG
     BIOS Date:                05/02/06
     Chipset Name:             NVIDIA nForce3 250Gb
     Chipset Vendor:           Nvidia Corp
     Chipset:                  nForce3 CPU to PCI Bridge
     Southbridge Vendor:       Nvidia Corp
     Southbridge:              nForce3 CPU to ISA Bridge
  System Enclosure
     Manufacturer:
     Type:                     Desktop
     Version:
     Serial Number:
     Asset Tag:
     Boot-up State:            Unknown
     Power Supply State:       Unknown
     Thermal State:            Unknown
     Security Status:          Unknown

                  +-----------------------------------------+
                  |                  CPU                    |
                  +-----------------------------------------+
  CPU
     Processor:                AMD Athlon 64 2800+
     Coprocessor:              Internal
     CPU Clock:                2402.9 MHz
     Level 1 Cache:            64+64 kB (data+instr.)
     Level 2 Cache:            512 kB
     FSB Clock:                267.0 MHz
     Multiplier:               9.0
     Platform ID:              Socket 754
     Vendor:                   AuthenticAMD
     Processor Name:           AMD Athlon(tm) 64 Processor 2800+
     Processor Type:           Original OEM Processor
     CPUID:                    Family: 15, Model: 12, Stepping: 0
     Ext. Family/Model:        Family: 0, Model: 0
     CPU Signature:            00000FC0h
     Brand ID:                 Athlon 64 2800+ (0106h)
     Logical CPU Count:        HTT Not Supported
     Max CPUID Level:          1
     Max ExtCPUID Level:       80000018h
     Code Name:                Newcastle (0.13mk)
     Core Stepping:            DH-CG
     MSR C0010015h:            00000000h:0A000000h
     MSR C0010042h:            00000202h:000A0A0Ah
  Instruction Set
     Floating-Point Unit On-Chip:         [X]
     IA MMX Technology:                   [X]
     SSE Instruction Set:                 [X]
     SSE2 Instruction Set:                [X]
     SSE3 Instruction Set:                [ ]
     Supplemental SSE3 Instruction Set:   [ ]
     SSE4.1 Instruction Set:              [ ]
     SSE4.2 Instruction Set:              [ ]
     Advanced Vector Extensions (AVX):    [ ]
     FMA Instructions Set:                [ ]
     AES Instructions Set:                [ ]
     Intel Extended Memory 64 Tech.:      [ ]
     Intel Architecture - 64 (IA-64):     [ ]
     AMD MMX Instruction Extensions:      [X]
     AMD 3DNow! Instructions:             [X]
     AMD 3DNow! Extensions:               [X]
     AMD 3DNow! Prefetch:                 [ ]
     AMD SSE4A Extensions:                [ ]
     AMD SSE5 Extensions:                 [ ]
     AMD Misaligned SSE:                  [ ]
     AMD64 Architecture:                  [X]
     Cyrix Extended MMX:                  [ ]
     CMPXCHG8 Instruction Supported:      [X]
     CMPXCHG16 Instruction Supported:     [ ]
     Fast System Call:                    [X]
     Conditional Move Instruction:        [X]
     CLFLUSH Insruction Supported:        [X]
     Fast Save and Restore:               [X]
     Monitor/MWAIT Instructions:          [ ]
     SYSCALL/SYSRET Instructions:         [X]
     LAHF/SAHF Instructions:              [ ]
     POPCNT Insruction Supported:         [ ]
     XSAVE Insructions Supported:         [ ]
     OS Supports XSAVE Instructions:      [ ]
     PCLMULQDQ Instruction Supported:     [ ]
     MOVBE Insruction Supported:          [ ]
     AMD RDTSCP Insruction Supported:     [ ]
     AMD Fast Save and Restore:           [ ]
     AMD SKINIT, STGI, DEV Supported:     [ ]
  Processor Features
     Virtual Mode Extension:              [X]
     Debugging Extension:                 [X]
     Page Size Extension:                 [X]
     Time Stamp Counter:                  [X]
     Model Specific Registers:            [X]
     Physical Address Extension:          [X]
     Machine Check Exception:             [X]
     On-chip APIC Hardware Supported:     [X]
     Memory Type Range Registers:         [X]
     Page Global Enable:                  [X]
     Machine Check Architecture:          [X]
     Page Attribute Table:                [X]
     36-bit Page Size Extension:          [X]
     Processor Serial Number:             [ ]
     Debug Store:                         [ ]
     64-bit Debug Store:                  [ ]
     Self-Snoop:                          [ ]
     Hyper-Threading Technology:          [ ]
     Pending Break Enable:                [ ]
     CPL-Qualified Debug Store:           [ ]
     L1 Context ID:                       [ ]
     Send Task Priority Messages:         [ ]
     Direct Cache Access:                 [ ]
     Performance Capabilities MSR:        [ ]
     x2APIC Architecture:                 [ ]
     Advanced Bit Manipulation:           [ ]
     OS Visible Workaround:               [ ]
     Instruction Based Sampling:          [ ]
     Intel Virtualization Technology:     [ ]
     Intel Trusted Execution Technology:  [ ]
     Intel Turbo Boost Technology:        [ ]
     AMD No-execute Page Protection:      [X]
     AMD Secure Virtual Machine:          [ ]
     AMD Model-Specific Registers:        [X]
     AMD Multiprocessing Capable:         [ ]
     AMD CMP Legacy Mode:                 [ ]
     AMD CR8 in Legacy Mode:              [ ]
     AMD Ext. APIC Register Space:        [ ]
     AMD Watchdog Timer:                  [ ]
     AMD 1-GB Large Page:                 [ ]
  Power Management
     ACPI Supported:                      [ ]
     Thermal Monitor Supported:           [ ]
     Thermal Monitor 2:                   [ ]
     Enhanced SpeedStep Technology:       [ ]
     Digital Thermal Sensor:              [ ]
     Operating Point Protection:          [ ]
     AMD Temperature Sensor:              [X]
     AMD Frequency ID Control:            [X]
     AMD Voltage ID Control:              [X]
     AMD Thermal Trip:                    [X]
     AMD Thermal Monitoring:              [ ]
     AMD Software Thermal Control:        [ ]
     AMD Invariant TSC:                   [ ]
     AMD 100MHz Multiplier Steps:         [ ]
     AMD Hardware P-State Control:        [ ]

                  +-----------------------------------------+
                  |                CPU Cache                |
                  +-----------------------------------------+
  Level 1 Instruction Cache
     Size:                     64 kB
     Associativity:            2-way
     Lines per Tag:            1
     Line Size:                64 byte
     TLB 4K Pages:
       Number of Entries:      32
       Associativity:          full
     TLB 2/4M Pages:
       Number of Entries:      8
       Associativity:          full
  Level 1 Data Cache
     Size:                     64 kB
     Associativity:            2-way
     Lines per Tag:            1
     Line Size:                64 byte
     TLB 4K Pages:
       Number of Entries:      32
       Associativity:          full
     TLB 2/4M Pages:
       Number of Entries:      8
       Associativity:          full
  Level 2 Cache
     Size:                     512 kB
     Associativity:            16-way
     Lines per Tag:            1
     Line Size:                64 byte
     Instr. TLB 4K Pages:
       Number of Entries:      512
       Associativity:          4-way
     Data TLB 4K Pages:
       Number of Entries:      512
       Associativity:          4-way
     Instr. TLB 2/4M Pages:
       Number of Entries:      0
       Associativity:          off
     Data TLB 2/4M Pages:
       Number of Entries:      0
       Associativity:          off

                  +-----------------------------------------+
                  |              CPU (SMBIOS)               |
                  +-----------------------------------------+
  Processor
     Processor Vendor:         AMD
     Processor Version:        AMD Athlon(tm) 64 Processor 2800+
     Current Speed:            2403 MHz
     External Clock:           267 MHz
     Voltage:                  1.5 V
     Processor Upgrade:        Socket 754
     Processor Status:         CPU Enabled
     Socket Designation:       Socket 754
     Processor Type:           Central Processor
     Processor Family:         AMD Opteron
     Processor ID1:            00000FC0h
     Processor ID2:            078BFBFFh
     Max Speed:                3000 MHz
     Socket Status:            CPU Socket Populated
     Structure Length:         20h

                  +-----------------------------------------+
                  |            CPU (SMBIOS) Cache           |
                  +-----------------------------------------+
  Level 1 Cache
     Installed Size:           128 kB
     Operational Mode:         Write Back
     Current SRAM Type:        Synchronous
     Status:                   Enabled
     Socket Designation:       Internal Cache
     Cache Socketed:           Not Socketed
     Location:                 Internal
     Maximum Cache Size:       128 kB
     Supported SRAM Type:      Synchronous
     Cache Speed:              Unknown
     Error Correction:         Unknown
     System Cache Type:        Unknown
     Associativity:            Unknown
     Structure Length:         13h
  Level 2 Cache
     Installed Size:           512 kB
     Operational Mode:         Write Back
     Current SRAM Type:        Synchronous
     Status:                   Enabled
     Socket Designation:       External Cache
     Cache Socketed:           Not Socketed
     Location:                 Internal
     Maximum Cache Size:       512 kB
     Supported SRAM Type:      Synchronous
     Cache Speed:              Unknown
     Error Correction:         Unknown
     System Cache Type:        Unknown
     Associativity:            Unknown
     Structure Length:         13h

                  +-----------------------------------------+
                  |                  BIOS                   |
                  +-----------------------------------------+
  BIOS
     Motherboard Vendor:       EPoX Computer Co., Ltd.
     Vendor URL:               www.epox.com
     BIOS Version:             Phoenix - AwardBIOS v6.00PG
     BIOS Model:               Model: FCh  SubModel: 01h  Revision: 00h
     BIOS Date:                05/02/06
     BIOS Copyright:           Phoenix Technologies, Ltd.- 04/23/90
     Motherboard ID:           05/02/2006 For nForce3 250 Chipset
     BIOS ID:                  05/02/2006-nForce-6A61CPAFC-00
     BIOS Type:                Medallion BIOS v6.00
     Bus Type:                 ISA/PCI
     Processor:                686
     Chipset:                  NVidia nForce3 150/250Gb
     Chipset ID:               nForce
     BIOS Revision:            00
     MP Specification Ver.:    1.4
     MP Table Address:         000Fh:0C00h
     Number of CPU/Cores:      1
     DMI/SMBIOS Version:       2.2
     DMI/SMBIOS Structures:    34
     DMI/SMBIOS Address:       000Fh:0000h
     APM Version:              Not Supported
  SMBIOS
     BIOS Vendor:              Phoenix Technologies, LTD
     BIOS Version:             6.00 PG
     BIOS Date:                05/02/2006
     BIOS ROM Size:            512 kB
     Starting Segment:         E000h
     Current Language:         n|US|iso8859-1
     Number of Languages:      3
     Structure Length:         13h
  Bus Supported
     PCI is Supported:                    [X]
     AGP is Supported:                    [X]
     USB is Supported:                    [X]
     ISA is Supported:                    [X]
     VLBus is Supported:                  [ ]
     MCA is Supported:                    [ ]
     EISA is Supported:                   [ ]
     PC Card is Supported:                [ ]
  Boot Options
     Selectable Boot:                     [X]
     Boot From CD:                        [X]
     ATAPI ZIP Drive Boot:                [X]
     LS-120 Boot:                         [X]
     BIOS Boot Specification:             [ ]
     Boot From PC Card:                   [ ]
     Network Service Boot Supported:      [ ]
     I2O Boot:                            [ ]
     1394 Boot:                           [ ]
  BIOS Features
     BIOS Characteristics:                [X]
     ACPI Supported:                      [X]
     PnP is Supported:                    [X]
     APM is Supported:                    [X]
     ESCD Support:                        [ ]
     Enhanced Disk Drive (EDD):           [X]
     BIOS is Upgradeable (Flash):         [X]
     BIOS ROM is Socketed:                [X]
     BIOS Shadowing is Allowed:           [X]
     Smart Battery Supported:             [ ]
     Targeted Content Distribution:       [ ]
     Int 13h - 5.25"/360kB Floppy:        [X]
     Int 13h - 5.25"/1.2MB Floppy:        [X]
     Int 13h - 3.5"/720kB Floppy:         [X]
     Int 13h - 3.5"/2.88MB Floppy:        [X]
     Int 5h, Print Screen Service:        [X]
     Int 9h, 8042 Keyboard Services:      [X]
     Int 14h, Serial Services:            [X]
     Int 17h, Printer Services:           [X]
     Int 10h, CGA/Mono Video Services:    [X]
     Int 13h - Floppy for NEC 9800:       [ ]
     Int 13h - Floppy for Toshiba:        [ ]
     NEC PC-98:                           [ ]
  Other SMBIOS Structures
     Memory Array Mapped Address (19)
     Memory Device Mapped Address (20)
     Memory Device Mapped Address (20)
     System Boot Information (32)

                  +-----------------------------------------+
                  |             PCI/AGP Devices             |
                  +-----------------------------------------+
  PCI/AGP
     PCI Bus Version:          2.10
     Number of PCI Buses:      3

  Bus: 00h, Device: 00h, Function: 00h
     Vendor (10DEh):           Nvidia Corp
     Device (00E1h):           nForce3 CPU to PCI Bridge
     Subsys Vendor (1695h):    Epox Computer Co Ltd
     Subsystem ID (100Ch):     Unknown
     Class (06h):              Bridge
     SubClass (00h):           PCI/CPU
     Revision:                 A1h
     Interface:                00h
  Device Properties
     Device Timing:            Fast
     Memory Access:            [X]
     I/O Access:               [ ]
     Bus Master:               [X]
     66 MHz Speed Support:     [X]
  Device Resources
     Memory Address:           C0000000h - CFFFFFFFh
  AGP Capabilities
     AGP Version:              3.0
     AGP Speed Supported:      4x 8x (Selected: 8x)
     Fast Write:               [X] enabled
     4GB Addressing:           [ ]
     Side Band Addressing:     [X] enabled

  Bus: 00h, Device: 01h, Function: 00h
     Vendor (10DEh):           Nvidia Corp
     Device (00E0h):           nForce3 CPU to ISA Bridge
     Subsys Vendor (1695h):    Epox Computer Co Ltd
     Subsystem ID (100Ch):     Unknown
     Class (06h):              Bridge
     SubClass (01h):           PCI/ISA
     Revision:                 A2h
     Interface:                00h
  Device Properties
     Device Timing:            Fast
     Memory Access:            [X]
     I/O Access:               [X]
     Bus Master:               [X]
     66 MHz Speed Support:     [X]
  Device Resources

  Bus: 00h, Device: 01h, Function: 01h
     Vendor (10DEh):           Nvidia Corp
     Device (00E4h):           nForce3 PCI SMB Controller
     Subsys Vendor (1695h):    Epox Computer Co Ltd
     Subsystem ID (100Ch):     Unknown
     Class (0Ch):              Serial
     SubClass (05h):           SMBus Controller
     Revision:                 A1h
     Interface:                00h
  Device Properties
     Device Timing:            Fast
     Memory Access:            [ ]
     I/O Access:               [X]
     Bus Master:               [ ]
     66 MHz Speed Support:     [X]
  Device Resources
     SMBus Port:               4C00h
     Base I/O Port:            0000E400h - 0000E41Fh
     Base I/O Port:            00004C00h - 00004C3Fh
     Base I/O Port:            00004C40h - 00004C7Fh
     System IRQ:               5
     Interrupt Pin:            INTA#

  Bus: 00h, Device: 02h, Function: 00h
     Vendor (10DEh):           Nvidia Corp
     Device (00E7h):           nForce3 OHCI USB Controller
     Subsys Vendor (1695h):    Epox Computer Co Ltd
     Subsystem ID (100Ch):     Unknown
     Class (0Ch):              Serial
     SubClass (03h):           USB
     Revision:                 A1h
     Interface:                10h
  Device Properties
     Device Timing:            Fast
     Memory Access:            [X]
     I/O Access:               [X]
     Bus Master:               [X]
     66 MHz Speed Support:     [X]
  Device Resources
     Memory Address:           DB004000h - DB004FFFh
     System IRQ:               5
     Interrupt Pin:            INTA#

  Bus: 00h, Device: 02h, Function: 01h
     Vendor (10DEh):           Nvidia Corp
     Device (00E7h):           nForce3 OHCI USB Controller
     Subsys Vendor (1695h):    Epox Computer Co Ltd
     Subsystem ID (100Ch):     Unknown
     Class (0Ch):              Serial
     SubClass (03h):           USB
     Revision:                 A1h
     Interface:                10h
  Device Properties
     Device Timing:            Fast
     Memory Access:            [X]
     I/O Access:               [X]
     Bus Master:               [X]
     66 MHz Speed Support:     [X]
  Device Resources
     Memory Address:           DB005000h - DB005FFFh
     System IRQ:               5
     Interrupt Pin:            INTB#

  Bus: 00h, Device: 02h, Function: 02h
     Vendor (10DEh):           Nvidia Corp
     Device (00E8h):           nForce3 EHCI USB 2.0 Controller
     Subsys Vendor (1695h):    Epox Computer Co Ltd
     Subsystem ID (100Ch):     Unknown
     Class (0Ch):              Serial
     SubClass (03h):           USB
     Revision:                 A2h
     Interface:                20h
  Device Properties
     Device Timing:            Fast
     Memory Access:            [X]
     I/O Access:               [ ]
     Bus Master:               [X]
     66 MHz Speed Support:     [X]
  Device Resources
     Memory Address:           DB000000h - DB0000FFh
     System IRQ:               5
     Interrupt Pin:            INTC#

  Bus: 00h, Device: 05h, Function: 00h
     Vendor (10DEh):           Nvidia Corp
     Device (00DFh):           Network Bus Enumerator
     Subsys Vendor (1695h):    Epox Computer Co Ltd
     Subsystem ID (100Ch):     Unknown
     Class (06h):              Bridge
     SubClass (80h):           PCI/Other
     Revision:                 A2h
     Interface:                00h
  Device Properties
     Device Timing:            Fast
     Memory Access:            [X]
     I/O Access:               [X]
     Bus Master:               [X]
     66 MHz Speed Support:     [X]
  Device Resources
     Memory Address:           DB001000h - DB001FFFh
     Base I/O Port:            0000B800h - 0000B807h
     System IRQ:               5
     Interrupt Pin:            INTA#

  Bus: 00h, Device: 06h, Function: 00h
     Vendor (10DEh):           Nvidia Corp
     Device (00EAh):           nForce3 AC'97 Audio Codec Interface
     Subsys Vendor (1695h):    Epox Computer Co Ltd
     Subsystem ID (100Dh):     Unknown
     Class (04h):              Multimedia
     SubClass (01h):           Audio
     Revision:                 A1h
     Interface:                00h
  Device Properties
     Device Timing:            Fast
     Memory Access:            [X]
     I/O Access:               [X]
     Bus Master:               [X]
     66 MHz Speed Support:     [X]
  Device Resources
     Base I/O Port:            0000BC00h - 0000BCFFh
     Base I/O Port:            0000C000h - 0000C07Fh
     Memory Address:           DB002000h - DB002FFFh
     System IRQ:               11
     Interrupt Pin:            INTA#
  AC'97/HDA Capabilities
     AC'97/HDA Codec Name:     Avance Logic ALC655
     Codec Enhancement:        No 3D Stereo Enhancement

  Bus: 00h, Device: 08h, Function: 00h
     Vendor (10DEh):           Nvidia Corp
     Device (00E5h):           nForce3 250 Parallel ATA Controller
     Subsys Vendor (1695h):    Epox Computer Co Ltd
     Subsystem ID (100Ch):     Unknown
     Class (01h):              Storage
     SubClass (01h):           IDE
     Revision:                 A2h
     Interface:                8Ah
  Device Properties
     Device Timing:            Fast
     Memory Access:            [ ]
     I/O Access:               [X]
     Bus Master:               [X]
     66 MHz Speed Support:     [X]
  Device Resources
     Base I/O Port:            0000F000h - 0000F00Fh

  Bus: 00h, Device: 0Ah, Function: 00h
     Vendor (10DEh):           Nvidia Corp
     Device (00E3h):           nForce3 250 Serial ATA Controller
     Subsys Vendor (1695h):    Epox Computer Co Ltd
     Subsystem ID (100Ch):     Unknown
     Class (01h):              Storage
     SubClass (01h):           IDE
     Revision:                 A2h
     Interface:                85h
  Device Properties
     Device Timing:            Fast
     Memory Access:            [ ]
     I/O Access:               [X]
     Bus Master:               [X]
     66 MHz Speed Support:     [X]
  Device Resources
     Base I/O Port:            000009F0h - 000009F7h
     Base I/O Port:            00000BF0h - 00000BF3h
     Base I/O Port:            00000970h - 00000977h
     Base I/O Port:            00000B70h - 00000B73h
     Base I/O Port:            0000DC00h - 0000DC0Fh
     Base I/O Port:            0000E000h - 0000E07Fh

  Bus: 00h, Device: 0Bh, Function: 00h
     Vendor (10DEh):           Nvidia Corp
     Device (00E2h):           nForce3 PCI to AGP Bridge
     Class (06h):              Bridge
     SubClass (04h):           PCI/PCI
     Revision:                 A2h
     Interface:                00h
  Device Properties
     Device Timing:            Medium
     Memory Access:            [X]
     I/O Access:               [X]
     Bus Master:               [X]
     66 MHz Speed Support:     [X]
  Device Resources
     Memory Address:           D8000000h - DAFFFFFFh
     Memory Address:           D0000000h - D7FFFFFFh

  Bus: 00h, Device: 0Eh, Function: 00h
     Vendor (10DEh):           Nvidia Corp
     Device (00EDh):           nForce3 PCI to PCI Bridge
     Class (06h):              Bridge
     SubClass (04h):           PCI/PCI
     Revision:                 A2h
     Interface:                00h
  Device Properties
     Device Timing:            Fast
     Memory Access:            [X]
     I/O Access:               [X]
     Bus Master:               [X]
     66 MHz Speed Support:     [X]
  Device Resources
     Base I/O Port:            A000h - AFFFh

  Bus: 00h, Device: 18h, Function: 00h
     Vendor (1022h):           Advanced Micro Devices (AMD)
     Device (1100h):           Athlon64/Opteron/Sempron (K8 Family) HyperTransport Technology Configuration
     Class (06h):              Bridge
     SubClass (00h):           PCI/CPU
     Revision:                 00h
     Interface:                00h
  Device Properties
     Device Timing:            Fast
     Memory Access:            [ ]
     I/O Access:               [ ]
     Bus Master:               [ ]
     66 MHz Speed Support:     [ ]
  Device Resources

  Bus: 00h, Device: 18h, Function: 01h
     Vendor (1022h):           Advanced Micro Devices (AMD)
     Device (1101h):           Athlon64/Opteron/Sempron (K8 Family) Address Map
     Class (06h):              Bridge
     SubClass (00h):           PCI/CPU
     Revision:                 00h
     Interface:                00h
  Device Properties
     Device Timing:            Fast
     Memory Access:            [ ]
     I/O Access:               [ ]
     Bus Master:               [ ]
     66 MHz Speed Support:     [ ]
  Device Resources

  Bus: 00h, Device: 18h, Function: 02h
     Vendor (1022h):           Advanced Micro Devices (AMD)
     Device (1102h):           Athlon64/Opteron/Sempron (K8 Family) DRAM Controller
     Class (06h):              Bridge
     SubClass (00h):           PCI/CPU
     Revision:                 00h
     Interface:                00h
  Device Properties
     Device Timing:            Fast
     Memory Access:            [ ]
     I/O Access:               [ ]
     Bus Master:               [ ]
     66 MHz Speed Support:     [ ]
  Device Resources

  Bus: 00h, Device: 18h, Function: 03h
     Vendor (1022h):           Advanced Micro Devices (AMD)
     Device (1103h):           Athlon64/Opteron/Sempron (K8 Family) Miscellaneous Control
     Class (06h):              Bridge
     SubClass (00h):           PCI/CPU
     Revision:                 00h
     Interface:                00h
  Device Properties
     Device Timing:            Fast
     Memory Access:            [ ]
     I/O Access:               [ ]
     Bus Master:               [ ]
     66 MHz Speed Support:     [ ]
  Device Resources

  Bus: 01h, Device: 00h, Function: 00h
     Vendor (10DEh):           Nvidia Corp
     Device (0041h):           GeForce 6800 [NV40.1]
     Subsys Vendor (1043h):    ASUSTeK Computer Inc
     Subsystem ID (817Ch):     V9999 Ultra Deluxe
     Class (03h):              Display
     SubClass (00h):           VGA
     Revision:                 A1h
     Interface:                00h
  Device Properties
     Device Timing:            Medium
     Memory Access:            [X]
     I/O Access:               [X]
     Bus Master:               [X]
     66 MHz Speed Support:     [X]
  Device Resources
     Memory Address:           D8000000h - D8FFFFFFh
     Memory Address:           D0000000h - D7FFFFFFh
     Memory Address:           D9000000h - D9FFFFFFh
     System IRQ:               11
     Interrupt Pin:            INTA#
  AGP Capabilities
     AGP Version:              3.0
     AGP Speed Supported:      4x 8x (Selected: 8x)
     Fast Write:               [X] enabled
     4GB Addressing:           [ ]
     Side Band Addressing:     [X] enabled

  Bus: 02h, Device: 0Bh, Function: 00h
     Vendor (1102h):           Creative Labs
     Device (0004h):           EMU10K2 Audio Chipset (SB Audigy Series)
     Subsys Vendor (1102h):    Creative Labs
     Subsystem ID (2005h):     Unknown
     Class (04h):              Multimedia
     SubClass (01h):           Audio
     Revision:                 04h
     Interface:                00h
  Device Properties
     Device Timing:            Medium
     Memory Access:            [ ]
     I/O Access:               [X]
     Bus Master:               [X]
     66 MHz Speed Support:     [ ]
  Device Resources
     Base I/O Port:            0000A000h - 0000A03Fh
     System IRQ:               5
     Interrupt Pin:            INTA#

                  +-----------------------------------------+
                  |              Memory Modules             |
                  +-----------------------------------------+
  Memory Slot 1
     Memory Type:              512MB PC3200 DDR SDRAM
     Manufacturer:             Samsung
     Module Type:              DIMM
     Number of Rows/Banks:     1 Rows, 4 Banks
     Module Attributes:        Unbuffered
     Error Checking:           None
     CAS# Latency:             3.0 (Cycle Time: 5.00ns/400MHz)
                               (Timings, CL-tRCD-tRP-tRAS: 3.0-3-3-8)
                               (tRC: 11, Access Time: 0.6ns)
     CAS# Latency:             2.5 (Cycle Time: 6.00ns/333MHz)
                               (Timings, CL-tRCD-tRP-tRAS: 2.5-3-3-7)
                               (tRC: 9, Access Time: 0.7ns)
     CS# Latency:              0
     WE# Latency:              1
     Refresh Rate:             Reduced (0.5x) 7.8 us, Self Refresh
     Data Width:               64 bits
     SDRAM Width:              x8
     Voltage Interface:        SSTL 2.5 V
     SPD Revision:             1.0
     Part Number:              M3 68L6523CUS-CCC
     Manufacture Date:         May 2006 (0616h)
     Serial Number:            F4253F48h
     Revision Code:            5343h
     EPP is Supported:         [ ]

  Memory Slot 2
     Memory Type:              512MB PC3200 DDR SDRAM
     Manufacturer:             Samsung
     Module Type:              DIMM
     Number of Rows/Banks:     1 Rows, 4 Banks
     Module Attributes:        Unbuffered
     Error Checking:           None
     CAS# Latency:             3.0 (Cycle Time: 5.00ns/400MHz)
                               (Timings, CL-tRCD-tRP-tRAS: 3.0-3-3-8)
                               (tRC: 11, Access Time: 0.6ns)
     CAS# Latency:             2.5 (Cycle Time: 6.00ns/333MHz)
                               (Timings, CL-tRCD-tRP-tRAS: 2.5-3-3-7)
                               (tRC: 9, Access Time: 0.7ns)
     CS# Latency:              0
     WE# Latency:              1
     Refresh Rate:             Reduced (0.5x) 7.8 us, Self Refresh
     Data Width:               64 bits
     SDRAM Width:              x8
     Voltage Interface:        SSTL 2.5 V
     SPD Revision:             1.0
     Part Number:              M3 68L6523DUS-CCC
     Manufacture Date:         August 2006 (0622h)
     Serial Number:            F42E570Eh
     Revision Code:            5344h
     EPP is Supported:         [ ]

                  +-----------------------------------------+
                  |             Memory (SMBIOS)             |
                  +-----------------------------------------+
  Physical Memory Array 1
     Maximum Capacity:         8192 MB
     Location:                 System Board or Motherboard
     Use:                      System Memory
     Memory Error Correct.:    None
     Memory Devices:           2
     Structure Length:         0Fh
  Memory Device 1
     Size:                     512 MB
     Form Factor:              DIMM
     Memory Type:              Unknown
     Device Locator:           A0
     Bank Locator:             Bank0/1
     Total Width:              64 bits
     Data Width:               64 bits
     Device Set:               00h
     Type Detail:              None
     Structure Length:         15h
  Memory Device 2
     Size:                     512 MB
     Form Factor:              DIMM
     Memory Type:              Unknown
     Device Locator:           A1
     Bank Locator:             Bank2/3
     Total Width:              64 bits
     Data Width:               64 bits
     Device Set:               00h
     Type Detail:              None
     Structure Length:         15h

                  +-----------------------------------------+
                  |                   HDD                   |
                  +-----------------------------------------+
  Primary/Master HDD
     HDD Model:                Maxtor 7L300R0
     HDD Size:                 286188 MB (279.48 GB)
     Interface Type:           Parallel ATA
     Geometry:                 Heads: 16, Sectors: 63, Tracks: 16383
     Compatibility:            ATA/ATAPI-7 revision 30
     Serial Number:            L61MYYGG
     Controller Revision:      BAJ41G20
     HDD Marketing Size:       300090 MB (300.09 GB)
     Buffer Size:              16384.0 kB
     Buffer Type:              Dual ported multi-sector buffer with a read caching
     HDD Temperature:          47 C (117 F)
     Reallocated Sectors:      0
     HDD Health Status:        Good
     ECC bytes:                57
     Security Erase Time:      None
     Enh. Security Erase:      None
     Current APM Value:        None
     Acoustic Management:      FEh (C0h Recommended) - Enabled
     ATA Controller Vendor:    Nvidia Corp
     ATA Controller Name:      nForce3 250 Parallel ATA Controller
     Device Location:          Primary/Master
  Transfer Modes
     PIO Mode Support:         4
     SW DMA Mode Support:      Not Supported
     MW DMA Mode Support:      2, Active: None
     UDMA Mode Support:        6 (UltraDMA/133), Active: 6 (UltraDMA/133)
     Sectors per Interrupt:    16, Active: 16
  HDD Features
     SATA NCQ Command:                    [ ]
     DMA Transfer:                        [X]
     LBA Supported:                       [X]
     Block Mode:                          [X]
     Double Word I/O:                     [ ]
     Standard Standby Timer:              [X]
     IORDY Supported:                     [X]
     IORDY may be Disabled:               [X]
     S.M.A.R.T.:                          [X] enabled
     S.M.A.R.T. Self-test:                [X] enabled
     S.M.A.R.T. Error Logging:            [X] enabled
     Security Mode Feature Set:           [X] disabled
     Removable Media:                     [ ]
     Power Management:                    [X] enabled
     PACKET Command:                      [ ]
     Write Cache:                         [X] enabled
     Look-ahead:                          [X] enabled
     Release Interrupt:                   [ ]
     Service Interrupt:                   [ ]
     Device Reset Command:                [ ]
     Host Protected Area:                 [X] enabled
     Write Verify Command:                [X] enabled
     Write Buffer Command:                [X] enabled
     Read Buffer Command:                 [X] enabled
     NOP Command:                         [X] enabled
     Identify Device DMA Command:         [ ]
     Download Microcode Command:          [X] enabled
     Read/Write DMA Queued:               [ ]
     CFA Feature Set:                     [ ]
     Advanced Power Management:           [X] disabled
     Removable Media Status:              [ ]
     Power-up in Standby:                 [ ]
     Set Features Req. to Spinup:         [ ]
     Set Max Security Extension:          [X] disabled
     Automatic Acoustic Management:       [X] enabled
     48-bit Address:                      [X] enabled
     Device Configuration Overlay:        [X] enabled
     Flush Cache Command:                 [X] enabled
     Flush Cache Ext Command:             [X] enabled
     Media Serial Number:                 [ ]
     Media Card Pass Through:             [ ]
     Streaming Feature Set:               [X] disabled
     General Purpose Logging:             [X] enabled
     Write DMA/Multiple FUA EXT:          [X] enabled
     Write DMA Queued FUA EXT:            [ ]
     World Wide Name:                     [ ]
  S.M.A.R.T.
     ID  | Attribute Name            |Threshold|Worst|Value| Raw Value
     ----+---------------------------+---------+-----+-----+-----------
     3   | Spin-up Time              |       63|  183|  184|      18579
     4   | Start/Stop Count          |        0|  253|  253|       1665
     5   | Reallocated Sectors Count |       63|  253|  253|          0
     6   | Read Channel Margin       |      100|  253|  253|          0
     7   | Seek Error Rate           |        0|  252|  253|          0
     8   | Seek Time Performance     |      187|  241|  246|      34507
     9   | Power On Hours Count      |        0|  247|  247|       6750
     10  | Spin-up Retry Count       |      157|  252|  253|          0
     11  | Recalibration Retries     |      223|  252|  253|          0
     12  | Drive Power Cycle Count   |        0|  249|  249|       1619
     192 | Power-Off Retract Cycle   |        0|  253|  253|          0
     193 | Load/Unload Cycle Count   |        0|  253|  253|          0
     194 | Drive Temperature         |        0|  253|   44|         47
     195 | Hardware ECC Recovered    |        0|  252|  253|       8381
     196 | Reallocation Event Count  |        0|  253|  253|          0
     197 | Current Pending Sectors   |        0|  253|  253|          0
     198 | Uncorrectable Sectors     |        0|  253|  253|          0
     199 | UltraDMA CRC Error Rate   |        0|  198|  199|          1
     200 | Write Error Rate          |        0|  252|  253|          0
     201 | Soft Read Error Rate      |        0|  252|  253|          0
     202 | Data Address Mark Errors  |        0|  252|  253|          0
     203 | Run Out Cancel            |      180|  252|  253|          0
     204 | Soft ECC Correction       |        0|  252|  253|          0
     205 | Thermal Asperity Rate     |        0|  252|  253|          0
     207 | Spin High Current         |        0|  252|  253|          0
     208 | Spin Buzz                 |        0|  252|  253|          0
     209 | Offline Seek Performance  |        0|  253|  253|          0
     210 | Vibration During Write    |        0|  252|  253|          0
     211 | Vibration During Read     |        0|  252|  253|          0
     212 | Shock During Write        |        0|  252|  253|          0

                  +-----------------------------------------+
                  |                  ATAPI                  |
                  +-----------------------------------------+
  Secondary/Master ATAPI
     ATAPI Model:              _NEC DVD_RW ND-3550A
     ATAPI Type:               DVD+-RW DL/CD-RW
     Interface Type:           Parallel ATA
     Physical Interface:       ATAPI
     ATAPI Name:               _NEC DVD_RW ND-3550A
     Vendor Specific:          05093000
     CD Read Speed:            48x (Current: 48x)
     CD Write Speed:           48x (Current: 48x)
     DVD Read Speed:           Current: 6x
     DVD Write Speed:          Current: 6x
     Buffer Size:              2048 kB
     Loading Mechanism:        Tray Type
     Rotation Control:         CLV
     Read Retry Count:         15
     Write Retry Count:        0
     Compatibility:            Unknown
     Serial Number:            63E1J06S211
     Controller Revision:      1.05
     Command DRQ Type:         Microprocessor DRQ
     Command Packet Size:      12 bytes
     ATA Controller Vendor:    Nvidia Corp
     ATA Controller Name:      nForce3 250 Parallel ATA Controller
     Device Location:          Secondary/Master
  Transfer Modes
     PIO Mode Support:         4
     SW DMA Mode Support:      Not Supported
     MW DMA Mode Support:      2, Active: None
     UDMA Mode Support:        2 (UltraDMA/33), Active: 2 (UltraDMA/33)
  Reading Features
     CD-R Disk Read:                      [X]
     CD-RW Disk Read:                     [X]
     DVD-ROM Disk Read:                   [X]
     DVD-RAM Disk Read:                   [ ]
     DVD-R Disk Read:                     [X]
     DVD-R DL Disk Read:                  [X]
     DVD-RW Disk Read:                    [X]
     DVD-RW DL Disk Read:                 [ ]
     DVD+R Disk Read:                     [X]
     DVD+R DL Disk Read:                  [X]
     DVD+RW Disk Read:                    [X]
     DVD+RW DL Disk Read:                 [ ]
     BD-ROM Disk Read:                    [ ]
     BD-R Disk Read:                      [ ]
     BD-RE Disk Read:                     [ ]
     HD DVD-ROM Disk Read:                [ ]
     HD DVD-RAM Disk Read:                [ ]
     HD DVD-R Disk Read:                  [ ]
     HD DVD-R DL Disk Read:               [ ]
     HD DVD-RW Disk Read:                 [ ]
     HD DVD-RW DL Disk Read:              [ ]
     Read Packet Using Method 2:          [X]
     Read Mode2 Form1 Sectors:            [X]
     Read Mode2 Form2 Sectors:            [X]
     Multisession Disk Read:              [X]
     READ-CD Command on AudioCD:          [X]
     Read Bar Code Capable:               [ ]
     Read Lead-in (CD-Text):              [X]
  Writing Features
     CD-R Disk Write:                     [X]
     CD-RW Disk Write:                    [X]
     DVD-RAM Disk Write:                  [ ]
     DVD-R Disk Write:                    [X]
     DVD-R DL Disk Write:                 [X]
     DVD-RW Disk Write:                   [X]
     DVD+R Disk Write:                    [X]
     DVD+R DL Disk Write:                 [X]
     DVD+RW Disk Write:                   [X]
     DVD+RW DL Disk Write:                [ ]
     BD-R Disk Write:                     [ ]
     BD-RE Disk Write:                    [ ]
     HD DVD-R Disk Write:                 [ ]
     HD DVD-R DL Disk Write:              [ ]
     HD DVD-RAM Disk Write:               [ ]
     HD DVD-RW Disk Write:                [ ]
     HD DVD-RW DL Disk Write:             [ ]
     Test Write Mode Support:             [X]
     Buffer Underrun Protection:          [X]
  Other Features
     Audio Play Support:                  [X]
     CD-DA Stream is Accurate:            [X]
     Composite Audio/Video:               [ ]
     Digital Output on Port 1:            [ ]
     Digital Output on Port 2:            [ ]
     Support Subcode R-W:                 [X]
     Support Subcode R-W D&C:             [ ]
     C2 Pointers Supported:               [X]
     ISRC Supported:                      [X]
     UPC Supported:                       [X]
  ATAPI Features
     DMA Transfer:                        [X]
     LBA Supported:                       [X]
     Block Mode:                          [ ]
     IORDY Supported:                     [X]
     IORDY may be Disabled:               [ ]
     ATA Software Reset:                  [ ]
     Overlap Operation:                   [ ]
     Command Queuing:                     [ ]
     Interleaving DMA:                    [ ]

  Secondary/Slave ATAPI
     ATAPI Model:              CD-W540E
     ATAPI Type:               CD-RW
     Interface Type:           Parallel ATA
     Physical Interface:       ATAPI
     ATAPI Name:               TEAC CD-W540E
     Vendor Specific:          09/30/02
     CD Read Speed:            48x (Current: 48x)
     CD Write Speed:           40x (Current: 40x)
     Buffer Size:              8192 kB
     Loading Mechanism:        Tray Type
     Rotation Control:         CLV
     Read Retry Count:         5
     Write Retry Count:        3
     Compatibility:            ATA/ATAPI-5 revision 19
     Serial Number:
     Controller Revision:      1.0H
     Command DRQ Type:         Accelerated DRQ
     Command Packet Size:      12 bytes
     ATA Controller Vendor:    Nvidia Corp
     ATA Controller Name:      nForce3 250 Parallel ATA Controller
     Device Location:          Secondary/Slave
  Transfer Modes
     PIO Mode Support:         4
     SW DMA Mode Support:      2, Active: None
     MW DMA Mode Support:      2, Active: None
     UDMA Mode Support:        2 (UltraDMA/33), Active: 2 (UltraDMA/33)
  Reading Features
     CD-R Disk Read:                      [X]
     CD-RW Disk Read:                     [X]
     DVD-ROM Disk Read:                   [ ]
     DVD-RAM Disk Read:                   [ ]
     DVD-R Disk Read:                     [ ]
     DVD-R DL Disk Read:                  [ ]
     DVD-RW Disk Read:                    [ ]
     DVD-RW DL Disk Read:                 [ ]
     DVD+R Disk Read:                     [ ]
     DVD+R DL Disk Read:                  [ ]
     DVD+RW Disk Read:                    [ ]
     DVD+RW DL Disk Read:                 [ ]
     BD-ROM Disk Read:                    [ ]
     BD-R Disk Read:                      [ ]
     BD-RE Disk Read:                     [ ]
     HD DVD-ROM Disk Read:                [ ]
     HD DVD-RAM Disk Read:                [ ]
     HD DVD-R Disk Read:                  [ ]
     HD DVD-R DL Disk Read:               [ ]
     HD DVD-RW Disk Read:                 [ ]
     HD DVD-RW DL Disk Read:              [ ]
     Read Packet Using Method 2:          [X]
     Read Mode2 Form1 Sectors:            [X]
     Read Mode2 Form2 Sectors:            [X]
     Multisession Disk Read:              [X]
     READ-CD Command on AudioCD:          [X]
     Read Bar Code Capable:               [ ]
     Read Lead-in (CD-Text):              [X]
  Writing Features
     CD-R Disk Write:                     [X]
     CD-RW Disk Write:                    [X]
     DVD-RAM Disk Write:                  [ ]
     DVD-R Disk Write:                    [ ]
     DVD-R DL Disk Write:                 [ ]
     DVD-RW Disk Write:                   [ ]
     DVD+R Disk Write:                    [ ]
     DVD+R DL Disk Write:                 [ ]
     DVD+RW Disk Write:                   [ ]
     DVD+RW DL Disk Write:                [ ]
     BD-R Disk Write:                     [ ]
     BD-RE Disk Write:                    [ ]
     HD DVD-R Disk Write:                 [ ]
     HD DVD-R DL Disk Write:              [ ]
     HD DVD-RAM Disk Write:               [ ]
     HD DVD-RW Disk Write:                [ ]
     HD DVD-RW DL Disk Write:             [ ]
     Test Write Mode Support:             [X]
     Buffer Underrun Protection:          [X]
  Other Features
     Audio Play Support:                  [X]
     CD-DA Stream is Accurate:            [X]
     Composite Audio/Video:               [ ]
     Digital Output on Port 1:            [ ]
     Digital Output on Port 2:            [ ]
     Support Subcode R-W:                 [X]
     Support Subcode R-W D&C:             [ ]
     C2 Pointers Supported:               [X]
     ISRC Supported:                      [X]
     UPC Supported:                       [X]
  ATAPI Features
     DMA Transfer:                        [X]
     LBA Supported:                       [X]
     Block Mode:                          [ ]
     IORDY Supported:                     [X]
     IORDY may be Disabled:               [X]
     ATA Software Reset:                  [ ]
     Overlap Operation:                   [ ]
     Command Queuing:                     [ ]
     Interleaving DMA:                    [ ]
     S.M.A.R.T.:                          [ ]
     S.M.A.R.T. Self-test:                [ ]
     S.M.A.R.T. Error Logging:            [ ]
     Security Mode Feature Set:           [ ]
     Removable Media:                     [ ]
     Power Management:                    [X] enabled
     PACKET Command:                      [X] enabled
     Write Cache:                         [ ]
     Look-ahead:                          [ ]
     Release Interrupt:                   [ ]
     Service Interrupt:                   [ ]
     Device Reset Command:                [X] enabled
     Host Protected Area:                 [ ]
     Write Verify Command:                [ ]
     Write Buffer Command:                [ ]
     Read Buffer Command:                 [ ]
     NOP Command:                         [X] enabled
     Identify Device DMA Command:         [ ]
     Download Microcode Command:          [ ]
     Read/Write DMA Queued:               [ ]
     CFA Feature Set:                     [ ]
     Advanced Power Management:           [ ]
     Removable Media Status:              [ ]
     Power-up in Standby:                 [ ]
     Set Features Req. to Spinup:         [ ]
     Set Max Security Extension:          [ ]
     Automatic Acoustic Management:       [ ]
     48-bit Address:                      [ ]
     Device Configuration Overlay:        [ ]
     Flush Cache Command:                 [ ]
     Flush Cache Ext Command:             [ ]
     Media Serial Number:                 [ ]
     Media Card Pass Through:             [ ]
     Streaming Feature Set:               [ ]
     General Purpose Logging:             [ ]
     Write DMA/Multiple FUA EXT:          [ ]
     Write DMA Queued FUA EXT:            [ ]
     World Wide Name:                     [ ]

                  +-----------------------------------------+
                  |              Storage (ASPI)             |
                  +-----------------------------------------+
  Host: 0, Target: 0, LUN: 0
     Device Name:              Kingston DataTraveler II+
     Size:                     491 MB (0.48 GB)
     Device Type:              Disk Drive
     Compatibility:            Not Standard
     Vendor Specific:
     Serial Number:
     Controller Revision:      1.13
     HDD Marketing Size:       515 MB (0.51 GB)
     Location:                 Host: 0, Target: 0, LUN: 0
     Manager ID:               ASPI for Windows
     Adapter ID:               PU20DISK
     Bus Width:                8-bit
     Address Width:            8-bit
  ASPI Device Features
     Removable Medium:                    Yes
     Read Cache:                          [ ]
     Write Cache:                         [ ]
     Read Reallocate:                     [ ]
     Write Reallocate:                    [ ]
     Terminate I/O Process:               [ ]
     Normal ACA:                          [ ]
     Hierarchical Support:                [ ]
     Embedded Array Controller:           [ ]
     Protection Information:              [ ]
     Enclosure Services:                  [ ]
     Multi-Ported Device:                 [ ]
     Medium Changer:                      [ ]
     Relative Addressing:                 [ ]
     Synchronous Transfer:                [ ]
     Linked Commands:                     [ ]
     Soft Reset:                          [ ]
     Quick Arbitration:                   [ ]

                  +-----------------------------------------+
                  |                  Drives                 |
                  +-----------------------------------------+
  BIOS Drives
     INT 13h Extensions:       1.x
  A:
     Drive Letter:             A:
     Drive Size:               1.44 MB
     Drive Type:               Floppy 1.44 MB (3.5")
     Cylinders:                80
     Heads:                    2
     Sectors:                  18
  C:
     Drive Letter:             C:
     Drive Size:               286189 MB
     Drive Type:               Fixed Disk
     Cylinders:                36483
     Heads:                    255
     Sectors:                  63
  D:
     Drive Letter:             D:
     Drive Size:               490 MB
     Drive Type:               Fixed Disk
     Cylinders:                490
     Heads:                    64
     Sectors:                  32
  H:
     Drive Letter:             H:
     Drive Type:               Optical Drive (MSCDEX Version: 2.95)
  I:
     Drive Letter:             I:
     Drive Type:               Optical Drive (MSCDEX Version: 2.95)

  Local Drives
  A:
     Drive Letter:             A:
     Drive Type:               Floppy 1.44 MB (3.5")
  C:[SYSTEM]
     Drive Letter:             C:
     Drive Type:               Fixed Disk
     Volume Label:             SYSTEM
     File System:              FAT16
     Volume Serial Number:     2255-1BEA
     Total Size:               2047.0 MB
     Free Space:               704.0 kB (0.0%)
  D:[UTILITIES]
     Drive Letter:             D:
     Drive Type:               Fixed Disk
     Volume Label:             UTILITIES
     File System:              FAT16
     Volume Serial Number:     2E4A-1BEB
     Total Size:               2047.0 MB
     Free Space:               7.5 MB (0.4%)
  E:[GAMES]
     Drive Letter:             E:
     Drive Type:               Fixed Disk
     Volume Label:             GAMES
     File System:              FAT16
     Volume Serial Number:     2D54-1BEC
     Total Size:               2047.0 MB
     Free Space:               21.2 MB (1.0%)
  F:[INSTALL]
     Drive Letter:             F:
     Drive Type:               Fixed Disk
     Volume Label:             INSTALL
     File System:              FAT16
     Volume Serial Number:     313D-1BED
     Total Size:               1890.2 MB
     Free Space:               436.6 MB (23.1%)
  G:[MUSIC]
     Drive Letter:             G:
     Drive Type:               Fixed Disk
     Volume Label:             MUSIC
     File System:              FAT32
     Volume Serial Number:     B9FE-C68F
     Total Size:               115.0 GB
     Free Space:               143.3 MB (0.1%)
  H:
     Drive Letter:             H:
     Drive Type:               Optical Drive
  I:
     Drive Letter:             I:
     Drive Type:               Optical Drive
  K:[KINGSTON]
     Drive Letter:             K:
     Drive Type:               Removable Disk
     Volume Label:             KINGSTON
     File System:              FAT16
     Volume Serial Number:     94C6-CB33
     Total Size:               491.2 MB
     Free Space:               228.1 MB (46.4%)

                  +-----------------------------------------+
                  |               USB Devices               |
                  +-----------------------------------------+
  USB Device 1
     Vendor (0951h):           Kingston Technology
     Device (1601h):           DataTraveler II Plus
     Manufacturer:             Kingston
     Product:                  DataTraveler II+
     Serial Number:            5B571621109C
     Device Version:           1.00
     Class (00h):              Unknown
     SubClass (00h):           Unknown
     Protocol (00h):           Unknown
     Configuration:
     USB Version:              2.00
     Speed:                    480 Mb/s
     Transfer Type:            Bulk
     Data Packet Size:         64 bytes
     Max Power:                200 mA
  Interface 1
     Class (08h):              Mass Storage
     SubClass (06h):           SCSI
     Protocol (50h):           Bulk (Zip)
     Interface:

                  +-----------------------------------------+
                  |              Plug and Play              |
                  +-----------------------------------------+
  Plug and Play
     PnP Version:              1.0
     Number of PnP Devices:    17

  Device Number 1
     PnP Device Name:          AT Interrupt Controller
     PnP Device ID:            PNP0000
     Base Type (08h):          System Peripheral
     SubType (00h):            Interrupt controller
     Node Size:                37 byte
  Device Resources
     I/O Port:                 0020h-0021h
     I/O Port:                 00A0h-00A1h
     System IRQ:               2 - High True Edge

  Device Number 2
     PnP Device Name:          AT DMA Controller
     PnP Device ID:            PNP0200
     Base Type (08h):          System Peripheral
     SubType (01h):            DMA controller
     Node Size:                69 byte
  Device Resources
     I/O Port:                 0000h-000Fh
     I/O Port:                 0081h-0083h
     I/O Port:                 0087h-0087h
     I/O Port:                 0089h-008Bh
     I/O Port:                 008Fh-0091h
     I/O Port:                 00C0h-00DFh
     DMA Channel:              4 - Type 8237 (8-bit)

  Device Number 3
     PnP Device Name:          AT Timer
     PnP Device ID:            PNP0100
     Base Type (08h):          System Peripheral
     SubType (02h):            System timer
     Node Size:                29 byte
  Device Resources
     I/O Port:                 0040h-0043h
     System IRQ:               0 - High True Edge

  Device Number 4
     PnP Device Name:          AT Real-Time Clock
     PnP Device ID:            PNP0B00
     Base Type (08h):          System Peripheral
     SubType (03h):            Real Time Clock
     Node Size:                29 byte
  Device Resources
     I/O Port:                 0070h-0071h
     System IRQ:               8 - High True Edge

  Device Number 5
     PnP Device Name:          IBM Enhanced keyboard controller (101/2-key)
     PnP Device ID:            PNP0303
     Base Type (09h):          Input Device
     SubType (00h):            Keyboard Controller
     Node Size:                37 byte
  Device Resources
     I/O Port:                 0060h-0060h
     I/O Port:                 0064h-0064h
     System IRQ:               1 - High True Edge

  Device Number 6
     PnP Device Name:          AT standard speaker sound
     PnP Device ID:            PNP0800
     Base Type (08h):          System Peripheral
     SubType (80h):            Other System device
     Node Size:                26 byte
  Device Resources
     I/O Port:                 0061h-0061h

  Device Number 7
     PnP Device Name:          Math Coprocessor
     PnP Device ID:            PNP0C04
     Base Type (0Bh):          CPU Type
     SubType (01h):            486 CPU
     Node Size:                29 byte
  Device Resources
     I/O Port:                 00F0h-00FFh
     System IRQ:               13 - High True Edge

  Device Number 8
     PnP Device Name:          System Board
     PnP Device ID:            PNP0C01
     Base Type (05h):          Memory
     SubType (00h):            RAM Memory
     Node Size:                90 byte
  Device Resources
     Memory Address:           00000000h-FFFFFFFFh RAM 8-bit Cacheble
     Memory Address:           FFFE0000h-FFFDFFFFh ROM 8/16-bit Cacheble
     Memory Address:           FEC00000h-FEBFFFFFh ROM 8/16-bit Cacheble
     Memory Address:           FEE00000h-FEDFFFFFh ROM 8/16-bit Cacheble
     Memory Address:           FEFFFC00h-FEFFFFFFh ROM 8/16-bit Cacheble
     Memory Address:           00100000h-000FFFFFh RAM 8-bit Cacheble

  Device Number 9
     PnP Device Name:          Motherboard registers
     PnP Device ID:            PNP0C02
     Base Type (08h):          System Peripheral
     SubType (80h):            Other System device
     Node Size:                66 byte
  Device Resources
     Memory Address:           000F0000h-000F3FFFh ROM 8/16-bit Cacheble Shadow
     Memory Address:           000F4000h-000F7FFFh ROM 8/16-bit Cacheble Shadow
     Memory Address:           000F8000h-000FFFFFh ROM 8/16-bit Cacheble Shadow
     Memory Address:           000D5800h-000D7FFFh ROM 8/16-bit Cacheble Shadow

  Device Number 10
     PnP Device Name:          PCI Bus
     PnP Device ID:            PNP0A03
     Base Type (06h):          Bridge Controller
     SubType (04h):            PCI Bridge
     Node Size:                42 byte
  Device Resources
     I/O Port:                 0294h-0297h
     I/O Port:                 04D0h-04D1h
     I/O Port:                 0CF8h-0CFFh

  Device Number 11
     PnP Device Name:          PS/2 Port for PS/2-style Mice
     PnP Device ID:            PNP0F13
     Base Type (09h):          Input Device
     SubType (02h):            Mouse Controller
     Node Size:                26 byte
  Device Resources
     System IRQ:               12 - High True Edge

  Device Number 12
     PnP Device Name:          16550A-compatible COM port
     PnP Device ID:            PNP0501
     Base Type (07h):          Communications
     SubType (00h):            RS-232 Serial port
     Node Size:                69 byte
  Device Resources
     I/O Port:                 03F8h-03FFh
     System IRQ:               4 - High True Edge

  Device Number 13
     PnP Device Name:          PC standard floppy disk controller
     PnP Device ID:            PNP0700
     Base Type (01h):          Mass Storage
     SubType (02h):            Floppy Controller
     Node Size:                64 byte
  Device Resources
     I/O Port:                 03F0h-03F5h
     I/O Port:                 03F7h-03F7h
     System IRQ:               6 - High True Edge
     DMA Channel:              2 - Type 8237 (8-bit)

  Device Number 14
     PnP Device Name:          Standard LPT printer port
     PnP Device ID:            PNP0400
     Base Type (07h):          Communications
     SubType (01h):            AT Parallel port
     Node Size:                92 byte
  Device Resources
     I/O Port:                 0378h-037Fh
     I/O Port:                 0778h-077Bh
     System IRQ:               7 - High True Edge

  Device Number 15
     PnP Device Name:          16550A-compatible COM port
     PnP Device ID:            PNP0501
     Base Type (07h):          Communications
     SubType (00h):            RS-232 Serial port
     Node Size:                69 byte
  Device Resources
     I/O Port:                 0000h-FFFFh

  Device Number 16
     PnP Device Name:          MPU401 compatible
     PnP Device ID:            PNPB006
     Base Type (04h):          Multimedia
     SubType (01h):            Audio controller
     Node Size:                60 byte
  Device Resources
     I/O Port:                 0330h-0331h
     System IRQ:               10 - High True Edge

  Device Number 17
     PnP Device Name:          Joystick/Game port
     PnP Device ID:            PNPB02F
     Base Type (04h):          Multimedia
     SubType (01h):            Audio controller
     Node Size:                69 byte
  Device Resources
     I/O Port:                 0201h-0207h
     I/O Port:                 0200h-0200h

                  +-----------------------------------------+
                  |            Physical Printers            |
                  +-----------------------------------------+
     LPT/PnP or USB printer not found

                  +-----------------------------------------+
                  |              Slots (SMBIOS)             |
                  +-----------------------------------------+
  Slot PCI
     Slot Type:                PCI
     Current Usage:            Available
     Data Bus Width:           32 bit
     Slot Designation:         PCI0
     Slot Length:              Long Length
     Slot ID:                  1
  Slot PCI
     Slot Type:                PCI
     Current Usage:            Available
     Data Bus Width:           32 bit
     Slot Designation:         PCI1
     Slot Length:              Long Length
     Slot ID:                  2
  Slot PCI
     Slot Type:                PCI
     Current Usage:            Available
     Data Bus Width:           32 bit
     Slot Designation:         PCI2
     Slot Length:              Long Length
     Slot ID:                  3
  Slot PCI
     Slot Type:                PCI
     Current Usage:            Available
     Data Bus Width:           32 bit
     Slot Designation:         PCI3
     Slot Length:              Long Length
     Slot ID:                  4
  Slot PCI
     Slot Type:                PCI
     Current Usage:            Available
     Data Bus Width:           32 bit
     Slot Designation:         PCI4
     Slot Length:              Long Length
     Slot ID:                  5
  Slot AGP
     Slot Type:                AGP
     Current Usage:            In Use
     Data Bus Width:           32 bit
     Slot Designation:         AGP
     Slot Length:              Long Length
     Slot ID:                  88

                  +-----------------------------------------+
                  |              Ports (SMBIOS)             |
                  +-----------------------------------------+
  Port 1 Other
     Int. Connector Type:      On Board IDE
     Ext. Connector Type:      None
     Port Type:                Other
     Int. Designator:          PRIMARY IDE
     Ext. Designator:
  Port 2 Other
     Int. Connector Type:      On Board IDE
     Ext. Connector Type:      None
     Port Type:                Other
     Int. Designator:          SECONDARY IDE
     Ext. Designator:
  Port 3 8251 FIFO Compatible
     Int. Connector Type:      On Board Floppy
     Ext. Connector Type:      None
     Port Type:                8251 FIFO Compatible
     Int. Designator:          FDD
     Ext. Designator:
  Port 4 Serial Port 16450 Compatible
     Int. Connector Type:      9 Pin Dual Inline (pin 10 cut)
     Ext. Connector Type:      DB-9 pin male
     Port Type:                Serial Port 16450 Compatible
     Int. Designator:          COM1
     Ext. Designator:
  Port 5 Serial Port 16450 Compatible
     Int. Connector Type:      9 Pin Dual Inline (pin 10 cut)
     Ext. Connector Type:      DB-9 pin male
     Port Type:                Serial Port 16450 Compatible
     Int. Designator:          COM2
     Ext. Designator:
  Port 6 Parallel Port ECP/EPP
     Int. Connector Type:      DB-25 pin female
     Ext. Connector Type:      DB-25 pin female
     Port Type:                Parallel Port ECP/EPP
     Int. Designator:          LPT1
     Ext. Designator:
  Port 7 Keyboard Port
     Int. Connector Type:      PS/2
     Ext. Connector Type:      PS/2
     Port Type:                Keyboard Port
     Int. Designator:          Keyboard
     Ext. Designator:
  Port 8 Mouse Port
     Int. Connector Type:      PS/2
     Ext. Connector Type:      PS/2
     Port Type:                Mouse Port
     Int. Designator:          PS/2 Mouse
     Ext. Designator:
  Port 9 USB
     Int. Connector Type:      None
     Ext. Connector Type:      Other
     Port Type:                USB
     Int. Designator:
     Ext. Designator:          USB0

                  +-----------------------------------------+
                  |                 Monitor                 |
                  +-----------------------------------------+
     PnP monitor not found

                  +-----------------------------------------+
                  |                  Video                  |
                  +-----------------------------------------+
  Video
     Video Chip Vendor:        Nvidia Corp
     Video Chip:               GeForce 6800 [NV40.1]
     Subsystem Vendor:         ASUSTeK Computer Inc
     Subsystem ID:             V9999 Ultra Deluxe
     Video Memory Size:        128 MB
     Bus Type:                 AGP
     VESA OEM String:          NVIDIA
     VESA Version:             3.0
     Vendor Name:              NVIDIA Corporation
     Product Name:             nv40 Board - p212-0   Chip Rev
     OEM Software Version:     5.64
  VESA Power Management
     VESA PM Version:          1.0
     Standby:                  [X]
     Suspend:                  [X]
     Off:                      [X]
     Reduced On:               [ ]
  AGP Capabilities
     AGP Version:              3.0
     AGP Speed Supported:      4x 8x (Selected: 8x)
     Fast Write:               [X] enabled
     4GB Addressing:           [ ]
     Side Band Addressing:     [X] enabled
  VESA Modes
     Number | Mode  |Resolution|Colors| bpp| Features
     -------+-------+----------+------+----+----------
       100h | Graph |   640x400|   256|   8| Bank + LFB
       101h | Graph |   640x480|   256|   8| Bank + LFB
       102h | Graph |   800x600|    16|   4| Bank
       103h | Graph |   800x600|   256|   8| Bank + LFB
       104h | Graph |  1024x768|    16|   4| Bank
       105h | Graph |  1024x768|   256|   8| Bank + LFB
       10Eh | Graph |   320x200|   64k|  16| Bank + LFB
       10Fh | Graph |   320x200|   16M|  32| Bank + LFB
       111h | Graph |   640x480|   64k|  16| Bank + LFB
       112h | Graph |   640x480|   16M|  32| Bank + LFB
       114h | Graph |   800x600|   64k|  16| Bank + LFB
       115h | Graph |   800x600|   16M|  32| Bank + LFB
       117h | Graph |  1024x768|   64k|  16| Bank + LFB
       118h | Graph |  1024x768|   16M|  32| Bank + LFB
       130h | Graph |   320x200|   256|   8| Bank + LFB
       131h | Graph |   320x400|   256|   8| Bank + LFB
       132h | Graph |   320x400|   64k|  16| Bank + LFB
       133h | Graph |   320x400|   16M|  32| Bank + LFB
       134h | Graph |   320x240|   256|   8| Bank + LFB
       135h | Graph |   320x240|   64k|  16| Bank + LFB
       136h | Graph |   320x240|   16M|  32| Bank + LFB
       13Dh | Graph |   640x400|   64k|  16| Bank + LFB
       13Eh | Graph |   640x400|   16M|  32| Bank + LFB

                                [End of Report]
